|  |  |
| --- | --- |
| From: ARM Committee | ARM11-13.2.5 |
| To: ENG Committee(s) | 13 March 2020 |

LIAISON NOTE

Update of Recommendation E-110

RHYTHMIC CHARACTERS OF LIGHTS ON AIDS TO NAVIGATION

# Introduction

At ARM11 the new Guideline on Mobile Aids to Navigation was finalised by ARM and forwarded to Council for approval. For physical MAtoN fitted with lights a unique light character has been designed.

# Comments

Recommendation E-110 will need to be amended with the specific character designed for use on physical MAtoN fitted with lights.

ARM suggests that the new character is added at the end of Table 3, below the entry for the EWMB. A suggested entry is provided below. Since the guideline has no number alotted at the time of writing this liaison note, the number reference below has ‘XXXX’ as placeholder.

|  |  |  |
| --- | --- | --- |
| MOBILE ATON | Flicker 1s (5 Hz) Eclipse 0.7s Flicker 1s (5Hz) Eclipse 0.5s Fl 1s Eclipse 0.5s Fl 1s Eclipse 3s. | Character defined in Guideline XXXX on Mobile AtoN.  Only the colour Yellow is used |

# Action requested

The committee is requested to:

1. When the Guideline on Mobile Aids to Navigation has been approved by council, amend Recommendation E-110 as described.