Document Revisions

*AISM* Association Internationale de Signalisation Maritime ***IALA***

**International Association of Marine Aids to Navigation and Lighthouse Authorities**

10, rue des Gaudines

78100 Saint Germain en Laye, France

Telephone: +33 1 34 51 70 01 Fax: +33 1 34 51 82 05

e-mail: [contact@iala-aism.org](mailto:contact@iala-aism.org) Internet: [www.iala-aism.org](http://www.iala-aism.org)

**IALA Guideline No. 1082**

**On**

**an Overview of AIS**

**Edition 1**

**Xxx 201X**

Revisions to the IALA Document are to be noted in the table prior to the issue of a revised document.

|  |  |  |
| --- | --- | --- |
| **Date** | **Page / Section Revised** | **Requirement for Revision** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Table of Contents

[Document Revisions 1](#_Toc412420836)

[Table of Contents 2](#_Toc412420837)

[Index of Tables 3](#_Toc412420838)

[Index of Figures 4](#_Toc412420839)

[An overview of AIS 5](#_Toc412420840)

[1 Introduction 5](#_Toc412420841)

[1.1 Scope 5](#_Toc412420842)

[1.2 What is AIS? 5](#_Toc412420843)

[1.3 Purpose of AIS 6](#_Toc412420844)

[1.3.1 AIS and radar 6](#_Toc412420845)

[1.4 Development of AIS 6](#_Toc412420846)

[1.4.1 SOLAS Requirement 6](#_Toc412420847)

[2 How does it operate 7](#_Toc412420848)

[2.1 Protocol for data transmission (language / sentences) 7](#_Toc412420849)

[2.1.1 Timing 8](#_Toc412420850)

[2.1.2 Position 8](#_Toc412420851)

[2.2 VHF data link 8](#_Toc412420852)

[2.3 Process for Data exchange 9](#_Toc412420853)

[2.4 Display of AIS data 9](#_Toc412420854)

[2.5 AIS Service 10](#_Toc412420855)

[2.6 Messages 10](#_Toc412420856)

[2.6.1 Standard messages 10](#_Toc412420857)

[2.6.2 Application-Specific Messages 12](#_Toc412420858)

[2.6.3 Management messages 12](#_Toc412420859)

[3 AIS Stations 13](#_Toc412420860)

[3.1 Mobile 15](#_Toc412420861)

[3.1.1 Shipborne 15](#_Toc412420862)

[3.1.2 AIS-SART -17](#_Toc412420863)

[3.1.3 AIS on SAR aircraft 18](#_Toc412420864)

[3.2 Fixed AIS stations 18](#_Toc412420865)

[3.2.1 AIS Base Stations 18](#_Toc412420866)

[3.2.2 AIS Repeaters 18](#_Toc412420867)

[3.2.3 AIS Aid to Navigation 18](#_Toc412420868)

[3.3 AIS Station Reporting Rate 19](#_Toc412420869)

[4 Basic AIS Service 19](#_Toc412420870)

[4.1 Coverage considerations 20](#_Toc412420871)

[4.2 AIS network 20](#_Toc412420872)

[4.3 Redundancy 20](#_Toc412420873)

[4.4 Vulnerability 20](#_Toc412420874)

[5 Use of AIS by IALA members 21](#_Toc412420875)

[6 Future Developments 21](#_Toc412420876)

[6.1 e-Navigation 21](#_Toc412420877)

[6.2 Satellite AIS 21](#_Toc412420878)

[6.3 Second Generation AIS 21](#_Toc412420879)

[6.4 AIS in GMDSS 21](#_Toc412420880)

[ANNEX A Time-line of the development of AIS 22](#_Toc412420881)

[ANNEX B AIS Stations BEHAVIOUR BY message type 24](#_Toc412420882)

[ANNEX C Data Broadcast by AIS station type 26](#_Toc412420887)

[ANNEX D AIS FUNTIONALITY by layer and STATION TYPE 30](#_Toc412420888)

[ANNEX E Acronyms 34](#_Toc412420889)

[ANNEX F AIS Documentation Overview 35](#_Toc412420890)

Index of Tables

[Table 1 Standard AIS messages 11](#_Toc441153512)

[Table 2 Overview of AIS stations 14](#_Toc441153513)

[Table 3 Comparison table – AIS Class A and AIS Class B 17](#_Toc441153514)

[Table 4 AIS Station Reporting Intervals 19](#_Toc441153515)

[Table 5 AIS Station Behaviour by Message Type 24](#_Toc441153516)

[Table 6 Data broadcast by AIS station type 26](#_Toc441153517)

[Table 7 AIS Functionality By Layer and Station Type 30](#_Toc441153518)

Index of Figures

[Figure 1 Protocol for AIS data transmission 9](#_Toc296962525)

[Figure 2 Display of AIS 10](#_Toc296962526)

[Figure 3 Representation of some types of AIS Stations 15](#_Toc296962527)

An overview of AIS

# Introduction

AIS was developed to provide automatic reporting between ships and to shore, which contributes to the safety of navigation and facilitates traffic management by exchanging information such as identity, position, time, course and speed, autonomously and continuously.

## Scope

This guideline provides an introduction to AIS at an overview level for shore authorities and references relevant documentation where further information can be found.

Further information on AIS documentation is provided at ANNEX F and is available on the IALA website.[[1]](#footnote-1)

## What is AIS?

AIS is a communications system using two worldwide dedicated channels in the VHF maritime mobile band, for the exchange of navigation data. There are numerous AIS devices, known as stations, which use an international open standard to communicate.

AIS stations are designed to operate autonomously (without interaction by ship or shore personnel) and may also be instructed to transmit in a different manner – for example may be interrogated (polled) or be commanded to transmit more frequently, or on a different frequency (assignment). AIS enables the automatic exchange of shipboard information from vessel sensors (dynamic data), as well as manually entered static and voyage related data[[2]](#footnote-2), between one vessel and another and between a vessel and a shore station(s).

AIS has been mandated as a shipboard carriage requirement for vessels under the revised Chapter V of the International Convention for the Safety of Life at Sea, 1974 (as amended) (SOLAS 74) section 19.2.4. in addition AIS is required domestically on non SOLAS vessels by some administrations.

The principal functions of AIS are to facilitate:

* Information exchange between vessels within VHF range of each other, increasing situational awareness;
* Information exchange between a vessel and a shore station, such as a VTS, to improve traffic management in congested waterways;
* Automatic reporting in areas of mandatory and voluntary reporting;
* Exchange of safety related information between vessels, and between vessels and shore station(s).

The development of AIS has expanded to include devices such as AIS for aids to navigation (AIS AtoN), AIS on search and rescue aircraft and AIS search and rescue transmitters[[3]](#footnote-3) (AIS-SART). Further explanation of the different AIS stations is included in section 4.

## Purpose of AIS

The AIS improves the safety of navigation and protection of the environment by assisting in the effective navigation of ships and the operation of VTS, by satisfying the following functional requirements*[[4]](#footnote-4)*:

*.l in a ship-to-ship mode for collision avoidance;*

*.2 as a means for littoral States to obtain information about a ship and its cargo; and*

*.3 as a VTS tool, i.e. ship-to-shore (traffic management).*

AIS provides for increased situational awareness which enables effective response to emergencies such as search and rescue (SAR) as well as environmental pollution. Additionally, AIS can provide data to identify trends or improvements in the provision of services to enhance navigational safety.

### AIS and radar

AIS information may be used in conjunction with radar information to facilitate:

* Vessel identification, heading, course over ground (COG) and speed over ground (SOG);
* Improved vessel tracking (no target swap);
* Wider geographical coverage;
* Greater positional accuracy, dependent on the position input sensor;
* Information in radar shadow area ('sees' around bends and behind islands);
* Near real time manoeuvring data;
* No loss of targets in sea, rain and snow clutter.

It is important to be aware that not all ships are required to carry AIS and that it is permissible for the AIS to be switched off if the master believes that the continual operation of AIS might compromise the safety or security of his/her ship, or if security incidents are imminent.*[[5]](#footnote-5)*

A vessel must inform the competent authority if it switches off its AIS whilst in a mandatory reporting area.

It should be noted that some data is entered or updated manually and so there is potential for incorrect entry and for the entered data to become out of date. This includes data related to static information (e.g. ship identity, dimension) and voyage related data (e.g. navigational status). Shore authorities should take the necessary action to ensure the integrity of the AIS data link and that the data transmitted on the link is correct.

## Development of AIS

AIS developed through the cooperative efforts of a number of different international organisations, including the IMO, the International Telecommunication Union (ITU), the International Association of Marine Aids to Navigation and Lighthouse Authorities (IALA) and the International Electrotechnical Commission (IEC).

AIS references to these international documents are included in ANNEX F.

# Use of AIS by IALA members

AIS can be an effective tool to assist aids to navigation authorities in a number of areas, as identified in the IALA Guideline 1050 on the management and monitoring of AIS information. For example, AIS can be used to:

* Display traffic on electronic navigational chart and radar display;
* Provide information to VTS centres;
* Monitor shipping routes including mandatory and recommended routes;
* Enable trend analysis of AIS data (number and sizes of different types of ships; use of routeing measures);
* Provide data for risk analysis;
* Provide data for long term planning;
* Provide data for marine accident investigation;
* Improve the effectiveness and efficiency of planning, management and maintenance of waterways including the provision of Aids-to-Navigation.

Additional information on the use of AIS by Authorities is provided in the latest edition of the IALA VTS Manual, IALA Recommendation V-128 on Operational And Technical Performance Requirements For VTS (Annex 3 – AIS), and, the IALA AIS Recommendations and Guidelines listed in Annex F.

# How does it operate

AIS stations communicate using a time-division multiple access (TDMA) communications scheme. Which means that the data link used is divided into a number of equal time slots which hold a set amount of data and are synchronised using GPS time. The primary methods by which AIS devices access the link (as detailed in ITU-R M.1371) are:

1. Self-Organised (SOTDMA) is the basic access method for mobile stations. Stations preannounce when they are going to transmit and plan their transmissions based on slot use information collected from other stations in order to prevent slot collisions (two stations picking the same slot to transmit their data packet).
2. Random Access (RATDMA)[[6]](#footnote-6) is used by AIS stations to access the link for unscheduled transmissions.
3. Fixed Access (FATDMA)[[7]](#footnote-7) is used by AIS stations that have a requirement to transmit data at predetermined intervals, and involves the reservation of particular slots for their exclusive use.
4. Carrier Sense (CSTDMA) – known as ‘polite’ behaviour is used by some mobile stations which can access the link only when they find an unused slot. These stations must listen to the beginning of a slot to detect occupancy and are therefore limited to a single slot transmission

Land AIS networks rely upon communication towers, referred to as Base Stations that manage the network in a similar manner to telephone ‘cell’ towers. When you experience a ‘dropped’ call on your mobile telephone it is usually because you are outside the cell (coverage area) or because the cell has too many other users. What makes AIS unique and very different from a mobile telephone network is the ability to ‘self-organise’. Simply, each AIS station is its own cell tower so its cell, or coverage area, moves with it. This is possible because the network is continuously self-organizing around the user, thus reducing the likelihood of ‘dropped call’ (undelivered AIS messages).

## Protocol for data transmission (language / sentences)

AIS uses TDMA protocols, this is the method used to communicate amongst stations, using pre-defined messages (sentences), which are exchanged between stations via two designated VHF frequencies[[8]](#footnote-8). The protocols, frequencies and the messages together are defined as the VHF data link (VDL). The VDL is similar to an internet email service where international compatibility is assured by a strict protocol, whatever the content of the message might be.

### Timing

Correct synchronisation of each users equipment is imperative to ensure proper functioning of the TDMA and is a critical part of the protocol for successful transmissions.

For AIS each minute of time (known as the ‘frame’) on each designated frequency is divided into 2250 slots, giving a total of 4500 for the two frequencies. Each frame of 2250 slots is repeated every minute. To ensure all units are synchronised, every AIS station contains a Global Navigation Satellite System receiver (GNSS – e.g. Global Positioning System (GPS)) which provides Universal Time Co-ordinated as a timing reference. If GNSS timing is lost, synchronisation is provided by other mobile units or AIS Base Stations in the area.

### Position

Although AIS relies on GPS for timing it may also obtain its position reference from an external source. Any interference or loss of the GNSS signal will impact AIS position data.


## VHF data link

The AIS has been designed for short range, VHF coverage, normally referred to as ‘line of sight’. Although most AIS messages only use one (1) slot, some can occupy up to five (5) consecutive time slots. The greater the number of slots used by a message, and the larger the number of vessels in a coverage area, the greater the potential for data packet (slot) collisions. Since most AIS base stations typically have a high antenna position, large coverage area, this may result in messages not being decoded from more distant AIS units in an area where there are a very large number of AIS stations operating. However data from these distant stations would continue to be transmitted and received correctly by closer AIS stations.

Administrations should organise the usage of the VDL by appropriate FATDMA[[9]](#footnote-9) reservations and consider the total load on the VDL before introducing additional services which rely on AIS.

The information exchanged via the VDL is safety related and the usage of the VDL should be monitored and controlled to safeguard its proper function and avoid overloading. IMO has highlighted this need in IMO Resolution MSC.347(91)

Even though there are potentially some scenarios in which data collisions may occur, the AIS is quite robust, and has been designed to work at high VDL loading.



1. Protocol for AIS data transmission

## Process for Data exchange


In addition to TDMA, AIS stations also use internationally adopted maritime digital interfaces and data sentences to exchange data amongst other devices, systems or networks (IEC 61162 / NMEA-183). This facilitates the display and use of AIS information on board the vessel and ashore, which enables the use of AIS to meet specific needs. On board the vessel the AIS provides data to the radar, ECDIS, chart-plotters etc., and ashore to VTS systems etc.

## Display of AIS data

AIS data can be displayed in different ways. AIS class A must have a Minimum Keyboard and Display (MKD), primarily intended for installation but displaying AIS target, name, bearing and range.

On vessels with AIS compliant navigational displays (IEC 62288), the manner in which targets are displayed depends on the type of AIS data;

* ship dynamic data are typically displayed as triangular shaped icons (see Figure 2)
* Ship static data is typically shown as a textbox
* Safety messages are also shown as a textbox
* diamond shaped



1. Display of AIS

## AIS Service

The AIS can be considered a maritime safety-related information service. The purpose of the AIS Service is to allow mariners and maritime administrations to interface with the different AIS stations on the VDL.

The AIS service provides a functional interface to access the available data from AIS stations. The purpose of this interface is to:

* facilitate the integration of the information from AIS into other applications;
* isolate the user from the technical details of the AIS technology and the way the AIS Service has been configured and implemented;
* allow for a simple point of control of what AIS data is shared with each user.

## Messages

The data exchange using AIS is based on well-defined messages which are listed in Table 1 below. The majority of the messages are concerned with the transfer of navigational information, however some messages are application specific or have system management functions, and are specifically described in the sections below.

### Standard messages

The standard messages used by AIS are given in the table below. These messages are approved by ITU for use by AIS. For further details see ITU-R M 1371.

1. Standard AIS messages

| Message ID# | Name | Description |
| --- | --- | --- |
| 1 | Position report | Scheduled position report |
| 2 | Position report | Assigned scheduled position report; |
| 3 | Position report | Special position report, response to interrogation; (Class A shipborne mobile equipment) |
| 4 | Base station report | Position, UTC, date and current slot number of base station |
| 5 | Static and voyage related data | Scheduled static and voyage related vessel data report; (Class A shipborne mobile equipment) |
| 6 | Binary addressed message | Binary data for addressed communication |
| 7 | Binary acknowledgement | Acknowledgement of received addressed binary data |
| 8 | Binary broadcast message | Binary data for broadcast communication |
| 9 | Standard SAR aircraft position report | Position report for airborne stations involved in SAR operations, only |
| 10 | UTC / date inquiry | Request UTC and date |
| 11 | UTC / date response | Current UTC and date if available |
| 12 | Safety related addressed text message | Safety related data for addressed communication |
| 13 | Safety related acknowledgement | Acknowledgement of received addressed safety related message |
| 14 | Safety related broadcast text message | Safety related data for broadcast communication |
| 15 | Interrogation | Request for a specific message type (can result in multiple responses from one or several stations) |
| 16 | Assignment mode command | Assignment of a specific reporting behaviour by competent authority using a base station to a single mobile station |
| 17 | DGNSS broadcast binary message | DGNSS corrections provided by a base station |
| 18 | Standard Class B equipment position report | Standard position report for Class B shipborne mobile equipment to be used instead of Messages 1, 2, 3 |
| 19 | Extended Class B equipment position report | Extended position report for class B shipborne mobile equipment; contains additional static information |
| 20 | Data link management message | Used by base station(s) to reserve slots |
| 21 | Aids-to-navigation report | Position and status report for aids-to-navigation |
| 22 | Channel management | Management of channels and transceiver modes by a base station |
| 23 | Group assignment command | Assignment of a specific reporting behaviour by competent authority using a base station to a specific group of mobiles |
| 24 | Static data report | Additional data assigned to an MMSI Part A: Name;(for any AIS station) Part B: Static Data (for Class B Shipborne mobile) |
| 25 | Single slot binary message | Short unscheduled binary data transmission (Broadcast or addressed) |
| 26 | Multiple slot binary message with Communi­cations State | Scheduled binary data transmission (Broadcast or addressed) |
| 27 | Long-range AIS broadcast message | Scheduled position report designed for satellite detection;  (Class A shipborne mobile station) |

### Application-Specific Messages (ASM)

Messages 6, 8, 25 and 26 provide a structure which can accommodate data suited for a specific application (e.g. meteorological and hydrological data, notifying of dangerous cargo, identifying a zone or a route, indicating pilotage requirements, etc.).

In addition to the message number, these applications are identified using a numbering system based on a unique three digit code known as the ‘Designated Area Code’ (DAC) and a two digit ‘Function Identifier’ (FI). This coding allows the correct use of the message if the necessary application software is available. These messages are similar to applications on a mobile telephone.

DAC 001, FI 00-09 identify international messages for technical purposes defined by ITU-R M.1371. DAC 001, FI 10-63 identify international messages defined and adopted by IMO, as described in SN.1/Circ.289.

DAC 010-999 identify regional functional messages, which may also be designated and adopted for use by administrations. Administrations are encouraged to register regional functional messages with IALA, who maintain the registry accessible from their website[[10]](#footnote-11).

Prior to developing a regional functional message, administrations should verify if a message with identical content is already on the registry (in use). These messages may be used outside the region, but the ‘ownership’ and control of the messages belong to the administration responsible for AIS in the area indicated by the DAC. Administrations are encouraged to use existing messages as appropriate with their registered DAC and FI. However, any changes to the content of an existing message would require a change to the DAC and FI and should be registered with IALA.

### Management messages

Management messages are used to control the behaviour of AIS stations and the use of the VDL. This functionality is performed solely by AIS base stations which should be controlled by a Competent Authority.

#### UTC and date inquiry (msg. 10) / response (msg. 11)

Stations may request / provide universal time coordinated information as needed.

#### Interrogation (msg. 15)

AIS stations may poll or interrogate other stations to request information other than UTC and date.

#### Assignment command (msg. 16)

Assignments are used by base stations to control the reporting interval of a mobile station. Message 16 will define both the slot and the increment for a given mobile station.

#### DGNSS broadcast (msg. 17)

This message may be transmitted by a base station which is connected to a DGNSS reference source, and configured to provide DGNSS data to other stations. Use of message 17 will correct the internal AIS GNSS. The system has not been designed to interface to the vessel’s GNSS (external to the AIS GNSS). The transmission of the differential broadcast can provide for more accurate positioning information where the AIS unit has an internal GNSS. In addition, the DGNSS reference source will warn the mariner and authorities about failures in the GNSS signal.

#### Data link management (msg. 20)

This message can be used by base stations to pre-announce the fixed allocation schedule (FATDMA) for one or more base stations and should be repeated as often as required. This message is used to reserve slots for a base station, or other fixed stations, to use. The mobile units will not use these slots. It is important to refresh the reservation of these slots, within the timeout period provided within the message, so that mobile units that are planning transmissions in future frames do not see the slots as available and new mobiles to the area receive the reservations in a timely manner. In addition, it is also important that slot reservation is coordinated so that the VDL remains available for the primary purpose of AIS, collision avoidance.[[11]](#footnote-12)

#### Channel management (msg. 22)

Channel management provides the ability to ‘require’ ships within a defined area to transmit and receive AIS on frequencies other than the two international AIS frequencies (AIS1, AIS2).

This can be accomplished by sending a channel management message on the existing AIS frequencies or on DSC channel 70. The alternate channel(s) chosen must be free from other VHF traffic.

This channel management can be used where the existing AIS frequencies are not available for use, if there is interference on existing AIS frequencies or in areas of high activity on the VDL.

Channel management must be effectively coordinated with adjoining stations to ensure that situational awareness in the transition zones is not lost.[[12]](#footnote-13)

It should be noted that experience has shown that not all units will respond properly to the DSC command to revert to the AIS channels, and the default timeout in the mobile unit is 30 days. Therefore IALA does not recommend the use of channel management.

#### Group assignment (msg. 23)

Group Assignment provides the ability to ‘require’ ships within a defined area and criteria to change their operating mode. The Group Assignment Command is transmitted by a base station when operating as a controlling entity. This command can be applied to a mobile station within the defined region and as selected by a mobile’s ‘Ship and Cargo Type’ or by ‘Station type’. The following operating parameters of a mobile station may be commanded using this message:

* transmit/ receive mode;
* reporting interval;
* the duration of a quiet time.

# AIS Stations

AIS is not solely used on board ship and can be grouped by ‘class’ (shipborne) and function. Shipborne AIS devices, which contribute the most to the flow of AIS information, are classified as either Class A or B. There are, however, other types of AIS stations that provide pertinent information or are used to manage AIS data. See Table 2.

1. Overview of AIS stations

For representation of some types of AIS see Figure 3.

|  |  |
| --- | --- |
| AIS Station | Description of AIS Station |
| AIS Class A[[13]](#footnote-14) | Class A stations are shipborne units which meet and are required on most commercial ships by the International Maritime Organisation (IMO). |
| AIS Class B | Class B stations are also shipborne units which are mainly compatible and very similar with AIS Class A but do not meet IMO technical or carriage requirements – primarily because they differ in power output and reporting rate. This Class has two variants based on the access scheme used: Carrier-Sense and Self-Organizing. |
| AIS base station | Base stations are designed for use by Competent authorities to manage the VDL and enable effective ship to shore / shore to ship transmission of information. They are the core of any AIS Service and can be networked to provide broad VTS or Coastal Surveillance coverage and overall maritime domain awareness. |
| AIS aids to navigation (AtoN) | AIS AtoN stations extend the visual or audible range of a traditional aid and provide current position or status; or they can provide ‘aid’ where a traditional aid does not yet exist, known as a virtual AtoN. |
| AIS-SART | Search and Rescue Transmitters (SART) are part of the Global Maritime Distress and Safety System (GMDSS). AIS Search and Rescue Transmitters (AIS-SARTs) can be used in lieu of radar SART. AIS-SARTs provide much greater range than radar SART. |
| AIS on Search and Rescue (SAR) Aircraft | AIS provides for a unique message intended for use by Search and Rescue Aircraft and to assist others in a SAR operation. |
| MOB-AIS | AIS Man Overboard Transmitters operate in a similar manner to the AIS-SART, but are used to indicate the position of an individual in the water. |
| EPIRB-AIS | Emergency Position Indicating Radio Beacons are part of the Global Maritime Distress and Safety System (GMDSS) and are based on a 406 MHz satellite detectable signal. An EPIRB-AIS also transmits an AIS message to assist with locating, and a 121.5 Mhz signal to assist with homing. |
| AIS Repeater | A station that repeats all non-system management messages to increase the range of the AIS VDL |



1. Representation of some types of AIS Stations

An indication of the data broadcast by each AIS station is provided in ANNEX C.

## Mobile

### Shipborne

Class A equipment complies with the IMO AIS performance standards. Class B are compatible with Class A and are fully compliant with ITU requirements, but, report less frequently and at a lower power than Class A. See Table 3.

#### Class A

During the installation of

The shipborne AIS units rely on inputs from the ship’s GNSS equipment (i.e. GPS), the heading device and rate of turn indicator. The requirement to feed this information to AIS is identified in SOLAS (e.g. SOLAS V/19.2.5 requires a gyro compass, or other means to determine and display heading, is provided as input into that AIS equipment).

Shipborne AIS units are also required to provide a number of interfaces to allow for integration of received information with a variety of onboard navigation equipment, including a minimum keyboard and display (MKD). This MKD is the mandated display tool for AIS Class A and provides for a minimum of three lines of data consisting of bearing, range and the name of a selected ship.

#### Class B

There can be two different variants of Class B stations, with different access methods (self-organizing TDMA and carrier-sense TDMA). Class B shipborne AIS stations are typically installed on non-SOLAS work craft and pleasure craft.

Class B units are not user configurable. Because of this, the units must be configured by the manufacturer or their representative (sales person) prior to use.

There is no requirement from IMO for carriage, installation or display of AIS Class B, however there are national requirements in some countries.

1. Comparison table – AIS Class A and AIS Class B

|  |  |  |  |
| --- | --- | --- | --- |
| Shipboard AIS Comparison | Class A  (SOLAS compliant) | Class B/CS | Class B/SO |
| Transmit Power | 12.5 watts (nominal) 1 watt[[14]](#footnote-17) (low power) | 2 watts | 5 watts (nominal) 1 watt14 (low power) |
| Major Communication Access Scheme | Self-organizing (SOTDMA) | Carrier-sense (CSTDMA) polite to Class A | Self-organising (SOTDMA) |
| Frequency Range &  Bandwidth | 156.025 - 162.025 MHz @ 25 kHz  DSC (156.525 MHz) required | 161.500 - 162.025 MHz @ 25 kHz  DSC (156.525 MHz) receive only | 161.500 - 162.025 MHz @ 25 kHz |
| Position Source and External Inputs | External GNSS, heading, rate of turn indication required; AIS internal GNSS | AIS internal GNSS; heading optional; External GNSS optional | External GNSS, heading, rate of turn indication required; AIS internal GNSS |
| Display / Digital Interfaces | Minimum keyboard display (MKD); multiple input-output ports and single output | Optional | Optional |
| Safety Text Messaging | Receive and transmit | Transmit optional, and only preconfigured. | Transmit optional, and only preconfigured. |

### AIS-SART

A Search And Rescue Transponder (AIS-SART) is used in the final stages of the execution of a search to respond to the ‘locating’ element of the Global Maritime Distress and Safety System (GMDSS). An AIS-SART is capable of transmitting messages that indicate the position (Message 1) and safety information (Message 14) of a unit in distress and is compatible with existing AIS installations[[15]](#footnote-18). The station will transmit a safety related text message, containing ‘SART ACTIVE’ during an emergency and ‘SART TEST’ when under test and are defined by the MMSI prefix ‘970’.

### AIS-MOB

AIS Man Over Board (MOB) transmitters operate in a similar manner to AIS-SART, but are used to indicate the position of an individual person. AIS-MOB transmit Message Type 1 with the Navigational status ‘14’, and a Message Type 14 which states: ‘MOB ACTIVE’ or ‘MOB TEST’; AIS-MOB are defined by the MMSI prefix ‘972’.

### EPIRB-AIS

Emergency Position Indicating Radio Beacons are part of the Global Maritime Distress and Safety System (GMDSS) and are based on a 406 MHz satellite detectable signal. EPIRBs use a 121.5 MHz for locating and an EPIRB-AIS also transmits an AIS Message Type 1 with the Navigational status ‘14’, and a Message Type 14 which states: ‘EPIRB ACTIVE’ or ‘EPIRB TEST’; EPIRB-AIS are defined by the MMSI prefix ‘974’.

### AIS on SAR aircraft

AIS can be fitted to aircraft to support search and rescue and safety of navigation. The position report for AIS on SAR aircraft includes information on altitude. AIS on SAR aircraft are identified by the MMSI prefix ‘111’. Optionally, administrations may use the seventh digit of the MMSI as follows: Fixed wing SAR aircraft may use 111MID1XX; SAR helicopters may use 111MID5XX.

## Fixed AIS stations

Fixed AIS stations refer to shore stations or AIS aid to navigation stations on lighthouses or other fixed locations.

### AIS Base Stations

The AIS base station is a device that is able to manage (see 3.6.3) the VDL. In highly trafficed areas the base station may benefit from a higher level application to fully take advantage of the benefits of AIS and management of the VDL. In addition to a fully functional base station able to control the VDLthere will be which can provide services to the mariner but

### AIS Repeaters

AIS repeaters can be used to extend the range of other AIS stations. The repeater must be within the range (often referred to as the footprint) of the other station to enable consistent repeat capability.

### AIS Aid to Navigation

An AIS unit can be fitted to an aid to navigation (AtoN) to provide positive identification, position and status of the AtoN. AIS AtoN may be fixed (i.e. attached to a lighthouse) or floating (i.e. attached to a buoy).

AIS AtoN stations are divided, from a technical point of view, as follows:

* Type 1. No receiver. Transmitter can only use pre-defined time slots (FATDMA), reserved by an AIS base station.
* Type 2. Receiver used for control functions - for configuration only. Transmitter uses pre-defined time slots only (see Type 1).
* Type 3. Full AIS receive capability typically used in an area without AIS base station coverage.

From an operational point of view AIS AtoN stations are identified as follows:

* Physical AIS AtoN. The AIS station is physically located on the AtoN.
* Synthetic AIS AtoN. AtoN messages for a specific AtoN are transmitted from a remote location (i.e. from another AtoN or a Base station).
* Virtual AIS AtoN. A remote AIS Station (another AtoN or a Base Station) transmit a message to identify an AtoN in a location where it does not physically exist. The virtual AIS AtoN can only be seen by other AIS units.

An AIS AtoN station may transmit ASMs, Safety Related Messages (e.g. AtoN is out of position or malfunctioning) and may also repeat any AIS-SART message received. In addition, the stations can work in a chaining environment to extend the range of AIS.[[16]](#footnote-19)

## AIS Station Reporting Rate

AIS reporting intervals vary by station as indicated in Table 4.

In addition to the nominal reporting frequency, the opportunity is available to poll vessels for updated information. A Competent Authority may use a base station to require mobile AIS devices to report more frequently.

1. AIS Station Reporting Intervals

| **Station Type** | | **Nominal Interval** |
| --- | --- | --- |
| Class B < 2 knots | | 3 minutes |
| Class A < 3 knots in ‘At anchor’ or ‘Moored’ status | | 3 minutes |
| Class B > 2 knots | | 30 seconds |
| Class A > 3 knots in ‘At anchor’ or ‘Moored’ status | | 10 seconds |
| Class A 0-14 knots | | 10 seconds |
| Class A 0-14 knots and changing course | | 31/3 seconds |
| Class B ‘SO’ 14-23 knots | | 15 seconds |
| Class A 14-23 knots | | 6 seconds |
| Class B ‘SO’ > 23 knots | | 5 seconds |
| Class A 14-23 knots and changing course; or > 23 knots | | 2 seconds |
| Search And Rescue Aircraft (airborne mobile equipment) | 10 seconds | |
| AIS Base Station | 10 seconds | |
| AIS Aid to Navigation | 3 minutes | |
| Transmissions of AIS Application Specific Messages | 3 minutes | |
| Transmissions of AIS Long Range Reports (message 27) | 6 minutes | |
| AIS-SART, AIS-MOB or EPIRB-AIS | 8 messages / minute | |

Note: Class B reporting interval is increased in high VDL loading situations.

# Basic AIS Service

The purpose and functions of the AIS can be expressed in terms of services provided to the recipient. The most fundamental ‘services’ of the AIS are called ‘Basic AIS Services’. The concept of ‘services’ make use of the information and features of the different AIS stations through the data transmitted over the VDL.

An AIS service can assist Administrations in meeting other IMO obligations such as providing a traffic image to assist VTS and addressing reporting requirements for traffic management schemes and ship reporting systems. It can assist in other shore-based safety-related services, including providing information to assist in the execution of a SAR operation. This AIS service consists of information delivery between ships and shore and vice versa.

Shore infrastructure for AIS normally includes a network connecting the different sources and users of AIS data within the area of responsibility of an Administration. The infrastructure can be as simple as a single AIS base station, with a way to display the data from the base station and a means to control or make use of the tools available in AIS (such as the messaging capability). The infrastructure can be thought of as a series of ‘layers’ that build up to provide control of the overall shore infrastructure. These layers include:

1. The Physical Shore Station (PSS) layer – consisting of one or more fixed AIS stations. (note – the PSS includes not only the actual AIS base station, but also all the connections, antenna, etc. required for the base station to actually operate).
2. The Logical Shore Station (LSS) layer – software that takes the AIS data from one or more PSS and delivers it, in a useable format, to the users of the AIS service. The LSS does not need to be co-located with the base station (the PSS).
3. The AIS Service Management (ASM) layer – the top layer of the system, where the system can be controlled. The ASM links to each base station, or group of base stations (PSS) through the software system (LSS) and controls the shore based AIS system. There is, however, a need to ensure reliable data transportation means between all association physical AIS shore stations.

The implementation of IALA guidelines for shore based AIS services (Annex F) allows for the creation of national, regional and international networks (e.g. Helcom, IALA-Net).

## Coverage considerations

AIS is designed to optimise close quarters ship to ship communications. When the VDL becomes congested ships should still be able to receive messages from those ships with the strongest signal (usually those ships that are in close proximity). Depending on the received coverage, shore stations may not necessarily receive messages from the strongest signal as some of these messages may actually collide with other messages.

When determining coverage area for AIS, shore authorities should take into account:

* traffic congestion;
* antenna design;
* antenna height and distance from the theoretical monitoring area;
* required availability for the application (e.g. VTS, coastal surveillance, traffic statistical analysis).

## AIS network

AIS data can be transferred over a fully transparent data transportation network (e.g. the internet). This process does not comprise any AIS-specific technology and can be integrated within an existing network.

## Redundancy

With increased reliance on reception of AIS data to support VTS, search and rescue and other uses, comes a need for high availability and reliability. This can be achieved through redundancy of system components.

## Vulnerability

All electronic devices, particularly radio equipment, are prone to radio frequency interference (RFI), particularly multi-pathing. Multi-pathing occurs when a radio signal (i.e. GPS signal) is received from two or more paths (e.g. bounced off a nearby large metal structure), this will commonly produce erroneous position calculations. AIS cannot and does not correct these errors—thus ghost targets arise. Such targets can also arise by malicious actions. AIS by design is non-secure, non-proprietary, open broadcast, as such it is not difficult to transmit deceptive or false broadcasts (spoof). AIS does provide for a means to verify targets, by being able to interrogate/poll any target for a new report should the user suspect spoofing. Those providing the false broadcasts are not likely to answer these polls with further reports because doing so could eventually reveal their location. False AIS reports can and should be expected of AIS and the AIS Service Manager layer may be able to provide automatic warning and verification if false targets are detected.

Spurious attacks or jamming of any VHF channels is relatively easy to do. VHF interference normally happens unintentionally or by poor design. Radio Direction Finding (RDF) equipment exists and is used to identify the source of interference, e.g. locate a stuck microphone on VHF-FM Ch 16.

AIS is a non-secure open broadcast system and the devices themselves do not share a common operating system. The internal operation of every AIS is of a proprietary design, thus not easy prey to hacking. This said, it is still imperative that Administrations actively monitor the VHF data link so as to be able to quickly identify intentional disruptions to AIS services and have procedures in place to mitigate them. Common internet cyber security measures should be adopted for any AIS systems that are networked.

# Future Developments

AIS is a versatile tool and, as experience is gained in the implementation and use of the various AIS stations, enhancements and other uses are being identified.

## e-Navigation

e-Navigation is an International Maritime Organization (IMO) led concept based on the harmonisation of marine navigation information and supporting shore services driven by user needs.

e-Navigation is currently defined as:

*e-Navigation is the harmonised collection, integration, exchange, presentation and analysis of maritime information onboard and ashore by electronic means to enhance berth to berth navigation and related services, for safety and security at sea and protection of the marine environment.*

IMO is working together with IALA to facilitate the e-Navigation concept for the mariner and the authorities. In this IALA is recommending future developments for AIS and other areas.

## Satellite AIS

Satellite AIS can extend coverage to the entire Exclusive Economic Zone (EEZ) or even globally, including ocean and remote coastal areas.

Satellite AIS is capable of receiving shipborne AIS today on existing frequencies. However, since these frequencies are shared with fixed and mobile stations, its ability to do so is affected by the very wide footprint of the satellite and the number of stations (fixed and mobile) within the footprint. Message Type 27 has been created to assist with the satellite detection of Class A AIS mobile units.

## VHF Data Exchange System (VDES)

There is a vision for a future VDES that will include AIS to also efficiently handle new applications as well as low volume data communications for e-Navigation.

The VDES will have new and improved features for both the shipboard and the shore-side. including services such as Marine Safety Information, electronic chart updates, automated ship reporting etc. and will also provide a more secure transmission medium.

## AIS in GMDSS

Although all AIS Class A devices have an integrated dedicated Digital Selective Calling receiver and, in initial devices, had the ability to transmit DSC tele-commands, they do not have the full functionality of a DSC radio that is part of GMDSS. This may change in the future as IMO contemplates GMDSS modernisation.

AIS Search and Rescue Transmitters (AIS-SART) are a locating device within GMDSS. Other Administrations recognise the Emergency Position Indicating Radio Beacon with AIS functionality (EPIRB-AIS) as distress locating devices.

1. Time-line of the development of AIS

The following provides a chronological overview of the development of AIS from initial international discussions to implementation of the IMO SOLAS carriage requirements. AIS continues to evolve.

|  |  |
| --- | --- |
| Sept. 1994 | IMO, 40th session of the safety of navigation committee (NAV40) - UK reported successful results of trials of a VHF DSC-based system and proposed that, to enhance the implementation of mandatory reporting systems and to assist in collision avoidance, ships should be fitted with an automatic identification transponder. NAV agreed to develop functional and operational requirements, as well as performance standards, and invited members to submit proposals to NAV41. |
| Sept. 1995 | NAV41 - Various proposals submitted including the VHF DSC by the UK; UHF and Satcom for long-range (France), VHF DSC gateways (USA) and a ‘blended’ approach using DSC, VHF and Inmarsat C for long range by Finland and Sweden. DSC was identified as a common factor, and was favoured for the overall implementation. The proposal by Finland and Sweden garnered interest, and IALA was invited to study the system with a view to developing standards to forward to ITU-R. |
| July 1996 | The requirements for short and long-range systems were recognised. The Automatic Identification System (or AIS) was discussed and two designs were under consideration. VHF DSC was considered the most suitable for VTS requirements, but the concept of the system was growing, and VHF DSC was not considered the most suitable collision avoidance, which would require an automatic broadcast system (as opposed to the concept of transponders which ‘squawk’ when requested to do so). The WG considered that a 2-step approach would enable early implementation of VHF/DSC, with later introduction of a system with more functionality when available. A liaison statement to ITU included 3 possible solutions: 2-Channel VHF Broadcast; 1200-baud gateway from DSC Ch 20; or UHF (using existing documentation in ITU-R M.825 – Characteristics of a transponder system using digital selective calling techniques for use with vessel traffic services and ship to ship identification.  The Finnish/Swedish proposal at that time, to use SOTDMA (Self-organising time division management access) was subject to patents, which raised some concerns over license fees. |
| Dec. 1996 | IMO Maritime Safety Committee (MSC67) - considered proposals for early implementation of VHF DSC, and for the VHF and Broadcast system being developed in tandem. However, after considerable debate, the 2-step approach was eventually abandoned in favour of a single, universal AIS to meet all requirements, and this was referred to NAV43. |
| July 1997 | NAV43 - carriage requirements were discussed and performance standards agreed. During discussions in the Technical Working Group (WG) the debate on technology intensified. It was agreed between delegations that they would not oppose the current ITU-R characteristics for a transponder system using VHF DSC (the ITU-R M.825-2).  However, at the request of Germany, Finland, South Africa, Sweden and the USA, IALA undertook to host a meeting to discuss and agree on a common approach for the technical characteristics. It was at this meeting that all involved agreed on the 4S system, using SOTDMA.  ITU World Radiocommunication Conference allocates two AIS VHF Channels. |
| 1998 | MSC 74 – IMO adopted the AIS performance standards in Resolution MSC.74(69  Recommendation ITU-R M1371 Ed. 0 published |
| 2000 | IMO amends the Safety of Life at Sea Convention, which amongst other things, establishes an AIS carriage requirement for tankers, passenger ships (regardless of size) and cargo ships of 300 gross tonnage or more; to be phased in from 2002 - 2008 (SOLAS Chap. V, Regulation 19.2.4) |
| 2001 | Recommendation ITU-R M1371 Ed. 1 published |
| 2002 | Following IMO diplomatic conference on maritime security the timeline for the mandatory adoption of AIS was shortened to 2004. |
| 2006 | Recommendation ITU-R M1371 Ed. 2 published |
| 2007 | Recommendation ITU-R M1371 Ed. 3 published |
| 2010 | Recommendation ITU-R M1371 Ed. 4 published |
| 2012 | World Radio Conference 2012 approves use of VHF channels 75 and 76 by AIS Class A mobile units for Message Type 27, and satellite detection of these messages. |
| 2014 | Recommendation ITU-R M1371 Ed. 5 published |
| 2015 | World Radio Conference 2015 approves use of VHF channels 27 and 28 for use of Application Specific Messaging. Additional channels for VDE were also approved. |
| 2015 | Recommendation ITU-R M. 2092 Ed. 0 published |

1. AIS Stations BEHAVIOUR BY message type
2. AIS Station Behaviour by Message Type

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Msg#** | **Class A** | | **Class B "SO"** | | **Class B  "CS"** | | **AtoN** | | **Base Station** | | **Repeater** | | **AIS-SART**  **MOB-AIS**  **EPIRB-AIS** | **SAR Aircraft\*** | | | **Limited Base Station\*** | |
| 1 | R | T | Rp | N | Rp | N | R3 | N | R | Tp | Rr | To | T | R | N | R | | N |
| 2 | R | T | Rp | N | Rp | N | R3 | N | R | Tp | Rr | T | N | R | N | R | | N |
| 3 | R | Ti | Rp | N | Rp | N | R3 | N | R | Tp | Rr | T | N | R | N | R | | N |
| 4 | R | N | Rp | N | Rp | N | R3 | N | R | Ti | Rr | T | N | R | N | R | | N |
| 5 | R | Ti | Rp | N | Rp | N | R3 | N | R | Tp | Rr | To | N | R | N | R | | N |
| 6 | R | T | R | T | Ro | To | R3 | To | R | Tv | Rr | To | N | R | To | R | | To |
| 7 | R | T | R | T | Ro | To | R3 | To | R | Tv | Rr | ? | N | R | T | R | | T |
| 8 | R | T | R | T | Ro | To | R3 | To | R | Tv | Rr | To | N | R | T | R | | T |
| 9 | R | N | R | N | Rp | N | R3 | N | R | Tp | Rr | T? | N | R | T | R | | N |
| 10 | R | T |  | N |  | N |  | N | R | Tv | Rr | T | N |  | T | R | | N |
| 11 | R | T |  | N |  | N |  | N | R | Tp | Rr | T | N |  | N | R | | N |
| 12 | R | T | Rp | T | Rp | N | R3 | To | R | Tv | Rr | T | N | R | T | R | | T |
| 13 | R | T | Rp | T |  | To | R3 | N | R | Tv | Rr | T | N | R | T | R | | T |
| 14 | R | T | R | T | Rp | To | R3 | To | R | Tv | Rr | T | T | R | T | R | | T |
| 15 | R | T | N | N | N | N |  | N | R | Tv | Rr | T | N | R | T | R | | T |
| 16 | R | N | R | N |  | N |  | N |  | Tv | Rr | T | N | R | N | R | | N |
| 17 | R | N | R | N | Ro | N | R3 | N | R | Tv | Rr | N | N | R | N | R | | N |
| 18 | R | N | R | Ti | Rp | Ti | R3 | N | R | Tp | Rr | T | N | R | N | R | | N |
| 19 | R | N | R | Ti | Rp | I | R3 | N | R | Tp | Rr | T | N | R | N | R | | N |
| 20 | R | N | R | N | Rp | N | R3 | N | R | Tv | Rr | T | N | R | N | R | | N |
| 21 | R | N | R | N | Rp | N | R3 | T | R | Tp | Rr | T | N | R | N | R | | T |
| 22 | R | N | R | N | Rp | N |  | N |  | Tv | Rr | T | N | R | N | R | | N |
| 23 | R | N | R | N | R | N |  | N |  | Tv | Rr | T | N | R | T | R | | N |
| 24A | R | Ti | R | I | Rp | Ti | R3 | N | R | Ti | Rr | T | N | R | Ti | R | | Ti |
| 24B | R | N Ti | R | I | Rp | Ti | R3 | N | R | Tp | Rr | T | N | R | I | R | | N |
| 25 | R | T | R | N | Rp | N | R3 | to | R | Tv | Rr | T | N | R | T | R | | N |
| 26 | R | T | R | T | Rp | N | R3 | N | R | Tv | Rr | T | N | R | T | R | | T |
| 27 |  | T |  | N |  | N |  | N | Ro | Tp |  | N | N |  | N |  | | N |

R Receives, processes, and forwards this message to the Presentation Interface (PI)

Rr Receives only, then repeats

R3 Only AIS ATON Type III receive message

Ro Reception is optional

Rp Reception, processing and portrayal is optional

I Transmits only if interrogated by a msg 15

T Transmits this message

Ti Transmits this message, and if interrogated by a msg 15

To Transmission is optional

Tp Capable of broadcasting this messages via a VDM PI input, however, not recommended

Tv Transits this message, and via a VDM PI input

N Not allowed/prohibited

\* AIS for SAR Aircraft and Limited Base Stations are still under development at IALA and/or IEC.

This table supersedes the information in IALA Guideline 1059. Specifications or behaviour in the tables are subject to changes that may arise during further development. These will be incorporated in future revisions of this guideline.

1. Data Broadcast by AIS station type
2. Data broadcast by AIS station type

| **EXACT DATA BROADCASTED VIA AIS BY STATION TYPE (Messages Used)**  Note: Not all data may be portrayed on shipboard or shore-side display systems | | Class A (1,5) | Class B/SO (18,19, 24B) | Class B/CS (18,24A,24B) | Base Station (4,24A) | Repeater Station | AIS-SART (1) | SAR A/C (9,5) | AtoN (21) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PARAMETER NAME** | **DESCRIPTION & FORMAT** |  |  |  |  |  |  |  |  |
| User ID | MMSI Number | X | X | X | X | X | X | X | X |
| Longitude | Longitude in 1/10 000 min (180º, East = positive (as per 2’s complement), West = negative (as per 2’s complement).  181= (6791AC0h) = not available = default) | X | X | X | X | X | X | X | X |
| Latitude | Latitude in 1/10 000 min (±90°, North = positive (as per 2’s complement), South = negative (as per 2’s complement). 91° (3412140h) = not available = default) | X | X | X | X | X | X | X | X |
| RAIM-Flag | RAIM (Receiver autonomous integrity monitoring) flag of electronic position fixing device; 0 = RAIM not in use = default; 1 = RAIM in use. See Table 50 in ITU-R M.1371-5. | X | X | X | X | X | X | X | X |
| Position Accuracy | The position accuracy (PA) flag should be determined in accordance with Table 50 in ITU-R M.1371-5.  1 = high (=<10 m)  0 = low (>10 m)  0 = default | X | X | X | X | X | X | X | X |
| Time Stamp | UTC second when the report was generated by the EPFS (0-59, or 60 if time stamp is not available, which should also be the default value, or 61 if positioning system is in manual input mode, or 62 if electronic position fixing system operates in estimated (dead reckoning) mode, or 63 if the positioning system is inoperative) | X | X | X |  | X | X | X | X |
| SOG | Speed over ground in 1/10 knot steps (0-102.2 knots)  1 023 = not available, 1 022 = 102.2 knots or higher | X | X | X |  | X | X | X |  |
| COG | Course over ground in 1/10° (0-3599). 3600 (E10h) = not available = default. 3 601- 4 095 should not be used | X | X | X |  | X | X | X |  |
| True Heading | Degrees (0-359) (511 indicates not available = default) | X | X | X |  | X | X |  |  |
| Type of Ship and/or Cargo Type | 0 = not available or no ship = default; 1-99 = as defined in § 3.3.2, Annex 8 in ITU-R M.1371-5; 100-199 = reserved, for regional use; 200-255 = reserved, for future use. Not applicable to SAR aircraft | X | X | X |  | X |  | X |  |
| Name | Maximum 20 characters 6 bit ASCII, as defined in Table 44 in ITU-R M.1371-5.  ‘@@@@@@@@@@@@@@@@@@@@’ = not available = default. For SAR aircraft, it should be set to ‘SAR AIRCRAFT NNNNNNN’ where NNNNNNN equals the aircraft registration number  For AtoN stations there is an additional 14 characters allowed. | X | X | X | X | X |  | X | X |
| Assigned Mode Flag | 0 = Station operating in autonomous and continuous mode=default; 1 = Station operating in assigned mode |  | X |  |  | X |  | X | X |
| DTE | Data terminal equipment (DTE) ready (0 = available, 1 = not available = default) (see § 3.3.1, Annex 8 in ITU-R M.1371-5) [The purpose of the data terminal equipment (DTE) indicator is to indicate to an application on the receiving side that, if set to available, the transmitting station conforms at least to the minimum keyboard and display requirements. | X | X |  |  | X |  | X |  |
| Call Sign | 7 × 6 bit ASCII characters, @@@@@@@ = not available = default. Craft associated with a parent vessel should use “A” followed by the last 6 digits of the MMSI of the parent vessel. (Examples of these craft include towed vessels, rescue boats, tenders, lifeboats and liferafts). | X | X | X |  | X |  | X |  |
| Special Manoeuver Indicator | 0 = not available = default,1 = not engaged in special manoeuvre 2 = engaged in special manoeuvre  (i.e. regional passing arrangement on Inland Waterway) | X |  |  |  | X | X |  |  |
| Rate of Turn  ROTAIS | 0 to +126 = turning right at up to 708 degrees per min or higher; 0 to -126 = turning left at up to 708 degrees per min or higher Values between 0 and 708 degrees per min coded by ROTAIS=4.733 SQRT(ROTsensor) degrees per min where ROT sensor is the Rate of Turn as input by an external Rate of Turn Indicator (TI). ROTAIS is rounded to the nearest integer value. +127 = turning right at more than 50 per 30s (No TI available) -127 = turning left at more than 50 per 30s (No TI available) -128 (80 hex) indicates no turn information available (default). ROT data should not be derived from COG information and is only required on vessels > 50,000GT. | X |  |  |  | X |  |  |  |
| Navigational Status | 0 = under way using engine, 1 = at anchor, 2 = not under command, 3 = restricted manoeuvrability, 4 = constrained by her draught, 5 = moored, 6 = aground, 7 = engaged in fishing, 8 = under way sailing, 9 = reserved for future amendment of navigational status for ships carrying DG, HS, or MP, or IMO hazard or pollutant category C (HSC), 10 = reserved for future amendment of navigational status for ships carrying DG, HS or MP, or IMO hazard or pollutant category A (WIG);  11 = towing astern, 12 = towing ahead, 13 = reserved for future use, 14 = AIS-SART (active), MOB-AIS (active), EPIRB-AIS (active)  15 = not defined = default (also used by AIS-SART, MOB-AIS, EPIRB-AIS under test) | X |  |  |  | X | X |  |  |
| Class B  Unit Flag | 0 = Class B SOTDMA unit; 1 = Class B ‘CS’ unit |  | X | X |  | X |  |  |  |
| Class B  Msg 22 Flag | 0 = No frequency management via Message 22 , operating on AIS1, AIS2 only; 1 = Frequency management via Message 22 |  | X | X |  | X |  |  |  |
| Class B  DSC Flag | 0 = Not equipped with DSC function  1 = Equipped with DSC function (dedicated or time-shared) |  | X | X |  | X |  |  |  |
| Class B Display Flag | 0 = No display available; not capable of displaying Message 12 and 14; 1 = Equipped with integrated display displaying Message 12 and 14 |  | X | X |  | X |  |  |  |
| Class B  Band Flag | 0 = Capable of operating over the upper 525 kHz band of the marine band; 1 = Capable of operating over the whole marine band (irrelevant if ‘Class B Message 22 flag’ is 0) |  | X | X |  | X |  |  |  |
| Type of Electronic Position Fixing Device | 0 = undefined (default); 1 = global positioning system (GPS); 2 = GLONASS; 3 = combined GPS/GLONASS; 4 = Loran-C; 5 = Chayka; 6 = integrated navigation system; 7 = surveyed; 8 = Galileo; 9 -14 = not used; 15 = internal GNSS | X | X |  | X | X |  | X | X |
| Overall Dimension / Reference for Position | Reference point for reported position. Also indicates the dimension of ship (m) (see Figure 41 and § 3.3.3, Annex 8 in ITU-R M.1371-5)  For SAR aircraft, the use of this field may be decided by the responsible administration. If used it should indicate the maximum dimensions of the craft. As default should A = B = C = D be set to ‘0’ | X | X | X |  | X |  | X | X |
| Vendor ID | Unique identification of the Unit by a number as defined by the manufacturer (option; ‘@@@@@@@’ = not available = default)  See Table 79A in ITU-R M.1371-5. |  | X | X |  | X |  |  |  |
| Maximum Present Static Draught | In 1/10 m, 255 = draught 25.5 m or greater, 0 = not available = default; in accordance with IMO Resolution A.851.  Not applicable to SAR aircraft, should be set to 0 | X |  |  |  | X |  |  |  |
| IMO Number | 1-999999999; 0 = not available = default – Not applicable to SAR aircraft.  0000000001 – 0000999999 not used  0001000000 – 0009999999 = valid IMO number  0010000000 – 1073741823 = official Flag State number. | X |  |  |  | X |  | X |  |
| ETA | Estimated time of arrival; MMDDHHMM UTC  Bits 19-16: month; 1-12; 0 = not available = default  Bits 15-11: day; 1-31; 0 = not available = default  Bits 10-6: hour; 0-23; 24 = not available = default  Bits 5-0: minute; 0-59; 60 = not available = default  For SAR aircraft, the use of this field may be decided by the responsible administration | X |  |  |  | X |  | X |  |
| Destination | Maximum 20 characters using 6-bit ASCII;  @@@@@@@@@@@@@@@@@@@@ = not available  For SAR aircraft, the use of this field may be decided by the responsible administration | X |  |  |  | X |  | X |  |
| AIS Version Indicator | 0 = station compliant with Recommendation ITU-R M.1371-1; 1 = station compliant with Recommendation ITU-R M.1371-3 (or later); 2 = station compliant with Recommendation ITU-R M.1371-5 (or later); 3 = station compliant with future editions | X |  |  |  | X |  | X |  |
| UTC Year | 1-9999; 0 = UTC year not available = default |  |  |  | X |  |  |  |  |
| UTC Month | 1-12; 0 = UTC month not available = default; 13-15 not used |  |  |  | X |  |  |  |  |
| UTC Day | 1-31; 0 = UTC day not available = default |  |  |  | X |  |  |  |  |
| UTC Hour | 0-23; 24 = UTC hour not available = default; 25-31 not used |  |  |  | X |  |  |  |  |
| UTC Minute | 0-59; 60 = UTC minute not available = default; 61-63 not used |  |  |  | X |  |  |  |  |
| UTC Second | 0-59; 60 = UTC second not available = default; 61-63 not used |  |  |  | X |  |  |  |  |
| Altitude Sensor | 0 = GNSS; 1 = barometric source |  |  |  |  |  |  | X |  |
| Altitude (GNSS) | Altitude (derived from GNSS or barometric (see altitude sensor parameter below)) (m) (0-4 094 m)  4 095 = not available, 4 094 = 4 094 m or higher |  |  |  |  |  |  | X |  |
| Type of aids-to-navigation | 0 = not available = default; refer to appropriate definition set up by IALA. See table 74 in ITU-R M.1371-5 |  |  |  |  | X |  |  | X |
| Off-position indicator | For floating AtoN, only: 0 = on position; 1 = off position |  |  |  |  | X |  |  | X |
| AtoN status | Reserved for the indication of the AtoN status; 00000000 = default. IALA Rec. A126 provides guidance on its use. |  |  |  |  | X |  |  | X |
| Virtual AtoN flag | 0 = default = real AtoN at indicated position; 1 = virtual AtoN, does not physically exist |  |  |  |  | X |  |  | X |
| Communication State | The communication state provides the following functions: (1) it contains information used by the slot allocation algorithm in the SOTDMA concept; and, (2) it also indicates the synchronisation state. See 3.3.7.2.2 SOTDMA communication state in ITU-R M.1371-5. |  |  |  |  | X |  |  |  |

Specifications or behaviour in the tables are subject to changes that may arise during further development.

These will be incorporated in future revisions of this guideline.

A repeater station repeats the following message types which contain the parameters indicated in the table above: 1, 2, 3, 5, 6, 7, 8, 12, 13, 14, 15, 18, 19, 21, 24, 25, 26.

1. AIS FUNTIONALITY by layer and STATION TYPE
2. AIS Functionality By Layer and Station Type

| **Functionality AIS Stations Type >>>** | | **Class A** | **Class B “SO”** | **Class B “CS”** | **AtoN** | **Base Station** | **AIS-SART  MOB-AIS EPIRB-AIS** | **Repeater** | **SAR Aircraft** | **Limited Base Station** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PHYSICAL LAYER** | Dual Channel | C | C | C | R, C3 | C | C | C | C | O |
| Single Channel | N | N | N | O, N3 | N | N | N | N | O |
| Full Frequency Range Capability | C | O | O | O | C | N | O | O | O |
| Receive / Transmit | C | C | C | N, C3 | C | N | C | C | C |
| Transmit Only | N | N | N | C, N3 | N | C | N | N | N |
| DSC Functionality | R | R | R | N | O | N | N | R | R |
| Operating Frequency Assignment Capability | C | O | O | N | N | N | N | C | O |
| Transmit Power in Watts: High (Nominal) Setting | 12.5 | 5 | 2 | M | M | M | 12.5 | M | 12.5 |
| Transmit Power in Watts: Low Power Setting | 1 | 1 | N | M | M | M | 2 | M | 1 |

| **Functionality AIS Stations Type >>>** | | **Class A** | **Class B “SO”** | **Class B “CS”** | **AtoN** | **Base Station** | **AIS-SARTMOB-AIS EPIRB-AIS** | **Repeater** | **SAR Aircraft** | **Limited Base Station** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LINK LAYER** | *TDMA Synchronisation* | | | | | | | | | |
| UTC Direct | C | C | O | C | C | C | C | C | C |
| UTC Indirect | C | O | O | N | C | N | C | C | O |
| Use Semaphore Synchronisation | C | O | N | N | C | N | C | C | N |
| Act as Semaphore | C | O | N | N | C | N | N | C | N |
| *Timing* | | | | | | | | | |
| Long Transmission Packets. No. of Slots | 3 | 3 | 12 | 3 | 5 | 1 | 3 | 3 | 2 |
| *Mode Of Operation* | | | | | | | | | |
| Autonomous | C | C | C | C | C | C | C | C | C |
| Assigned | C | C | C | N | N | N | N | C | C |
| Polled | C | C | C | N | C | N | N | C | C |
| Limitation Maximum Permissible Number of Slots Per Frame. | 20 | 31 | 31 | 20 | None | 10 | None | 20 | 20 |
| *VDL Access Schemes* |  | | | | | | | | |
| SOTDMA | C | C | N | N | N | N | N | C | N |
| RATDMA | C | C | N | N, C3 | O | N | C | C | C |
| ITDMA | C | C | N | N | N | N | N | C | C |
| FATDMA | N | N | N | C | C | N | O | N | N |
| CSTDMA | N | N | C | N, O3 | N | N | N | N | N |

| **Functionality AIS Stations Type >>>** | **Class A** | **Class B “SO”** | **Class B “CS”** | **AtoN** | **Base Station** | **AIS-SART  MOB-AIS EPIRB-AIS** | **Repeater** | **SAR Aircraft** | **Limited Base Station** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NETWORK** | *Channel Operation & Management* | | | | | | | | | |
| Default Channel Operation AIS 1 & AIS 2 | C | C | C | C | C | C | C | C | C |
| Channel Management Message 22 | C | C | C | N | N | N | N | C | C |
| DSC Telecommand | C | O | O | N | N | N | N | C | N |
| Manual Input | C | N | N | N | N | N | N | N | N |
| Presentation Interface | C | N | N | N | C | N | N | C | C |
| Reporting Modes A, B or C | N | N | N | C | N | C  [B Mode] | N | N | N |
| Frequency Agile | C | O | O | O | C | N | O | O | O |
| Slot Re-Use Data Link Congestion. | C | C | N | N, C3 | C | N | C | C | N |
| Long Range | C | N | N | N | N | N | N | N | N |

**C** Compulsory in any configuration

**O** Optional

**R** Receive only

**M** Manufacturer to determine

**N** Not allowed

***Notes***

1 The limitation is for messages 6, 8, 12 & 14.

2 Only if the Class B has a presentation port.

3 Only for AIS ATON Type III stations.

This table supersedes the information in IALA Guideline 1059. Specifications or behaviour in the tables are subject to changes that may arise during further development. These will be incorporated in future revisions of this guideline.

1. Acronyms

|  |  |
| --- | --- |
| AIS | Automatic Identification System |
| AIS 1 | AIS Default Channel 1 - 161.975 MHz (Ch. 87B//2087) |
| AIS 2 | AIS Default Channel 2 - 162.025 MHz (Ch. 88B/2088) |
| ASM | Application Specific Message |
| AIS-SART | AIS Search And Rescue Transmitter |
| AtoN | Aid to Navigation |
| CH | Channel |
| CSTDMA | Carrier-sense Time Division Multiple Access |
| DAC | Designated Area Code |
| DGNSS | Differential Global Navigation Satellite Service |
| DSC | Digital Selective Calling |
| ECDIS | Electronic Chart Display and Information System |
| ECS | Electronic Chart System |
| EPFS | Electronic Position Fixing System |
| EPIRB-AIS | Emergency Position Indicating Radio Beacon – AIS enabled |
| FATDMA | Fixed Access Time Division Multiple Access |
| FI | Function Identifier |
| GMDSS | Global Maritime Distress and Safety System |
| GNSS | Global Navigation Satellite Service |
| GPS | Global Positioning System |
| Gyro | Gyrocompass |
| IALA | International Association of Marine Aids to Navigation and Lighthouse Authorities |
| IEC | International Electrotechnical Commission |
| IMO | International Maritime Organization |
| ITDMA | Incremental Time Division Multiple Access |
| ITU-R | International Telecommunications Union –Radiocommunication Sector |
| ITU-R | ITU – Radiocommunications Sector |
| LSS | Logical AIS Shore Station |
| MID | Maritime Identification Digit |
| MKD | Minimum Keyboard and Display |
| MMSI | Maritime Mobile Service Identity |
| AIS-MOB | Man Overboard AIS device |
| MSG | AIS Message |
| MSC | IMO Maritime Safety Committee |
| NMEA | National Marine Electronics Association |
| PI | Presentation Interface |
| PSS | Physical AIS Shore Station |
| RATDMA | Random Access Time Division Multiple Access |
| RCC | Rescue Coordination Centre |
| RF | Radio Frequency |
| ROT | Rate of Turn |
| Rx | Receiver / receive |
| SAR | Search and Rescue |
| SART | Search And Rescue radar Transponder |
| SOG | Speed Over Ground |
| SOLAS | Safety Of Life At Sea |
| SOTDMA | Self-Organising Time Division Multiple Access |
| TDMA | Time Division Multiple Access |
| UTC | UTC Coordinated Universal Time |
| VDE | VHF Data Exchange |
| VDES | VHF Data Exchange System |
| VDL | VHF Data Link |
| VHF | Very High Frequency |
| VTS | Vessel Traffic Services |
| WG | Working Group |
| WGS84 | World Geodetic Survey 1984 |
| WRC | World Radiocommunication Conference |

1. AIS Documentation Overview

| Organisation | Doc Number | Doc Name | Status | Key points | Comments |
| --- | --- | --- | --- | --- | --- |
| IMO | Res. MSC.74(69)  12 May 1998 | Adoption Of New And Amended Performance Standards | In Force | Annex 3 – performance standards for AIS. | Provides the basic elements of what AIS should do. Introduces key terms – autonomous and continuous, static, dynamic and voyage related information. |
| IMO | Res. A.917(22)  29 Nov 2001 | Guidelines For The Onboard Operational Use Of Shipborne  Automatic Identification Systems (AIS) | In Force (amends Res. A.956(23)) | Provides the objectives of AIS, Description of shipborne AIS, data sets, reporting rates, operation, limitations, use of AIS for collision avoidance, AIS in VTS / SAR and Aids to Navigation (AtoN). | Reporting rates identified – from 2 sec to 3 min, depending on speed and activity for dynamic info; every 6 min for static info (or on demand) |
| IMO | Res. A.956(23)  26 Feb 2004 | Amendments To The Guidelines For The Onboard Operational Use Of Shipborne AIS  (Res. A.917(22)) | In Force (amends Res. A.917(22)) | Operation of Transceiver Unit – (para 21) Change includes security aspects – including option to turn off the AIS ‘or where security incidents are imminent’. | Notes that when a ship is in a Ship Reporting System (SRS) there is a requirement for the master to report the reason for turning off the AIS. |
| IMO | Res. MSC.99(73)  5 Dec 2000  Regulation 19, SOLAS | Adoption Of Amendments To The International Convention For The Safety Of Life At Sea, 1974, As Amended | In Force (amended by Diplomatic Conference) | Original implementation dates for AIS with incremental implementation starting 1 July 2002 and ending 1 July 2008. | Amended by **Diplomatic Conference on Maritime Security, 2002** - Original phased in implementation brought forward to completion by 1 July 2004. |
| IMO | Res. MSC.140(76)  5 Dec 2002 | Recommendation For The Protection  Of The AIS VHF Data Link (VDL) | Superceded by Res. MSC.347(91) | Related to the introduction of AIS Class B.  Recognises the ‘compelling need to ensure the integrity of the VHF Data Link (VDL)’ and puts onus on administrations | To Note:  .1 Class B AIS devices, as well as any device which transmits on the radio channels AIS 1 or AIS 2, should meet the appropriate requirements of Recommendation ITU-R M.1371 (series);  .2 Class B AIS devices should be approved by the Administration;  .3 Administrations should take steps necessary to ensure the integrity of the radio channels used for AIS in their waters. |
| IMO | MSC Circ.1062  16 Dec 2002 | Maintenance And Administration Of AIS Binary Messages | Superceded  Led to SN/Circ.236 then to SN.1 /Circ.289 | Notes the process for handing over responsibility for Binary Messages | Initially, IALA dealt with Binary Messages, in conjunction with ITU. The capability of binary messages has continued to evolve. |
| IMO | Res. MSC.246(83)  8 Oct 2007 | Adoption Of Performance Standards For Survival Craft AIS Search And Rescue Transmitters (AIS-SART) For Us In Search And Rescue Operations. | In Force | Provides performance standards for the AIS-SARTS. | Indicates that AIS-SARTs fitted on vessels conform to the identified performance standards. |
| IMO | [MSC. Circ.1252](http://www.navcen.uscg.gov/pdf/IMO_MSC1_Circ1252_AIS_testing.pdf)  20 Oct. 2007 | Guidelines On Annual Testing Of The Automatic Identification System (AIS) | In Force |  |  |
| IMO | Res. MSC.347(91)  30 Nov. 2012 | Recommendation For The Protection  Of The AIS VHF Data Link (VDL) | In Force (supersedes MSC.140(76)). | Related to the introduction of AIS Class B, AIS-SART and other AIS devices.  Recognises the ‘compelling need to ensure the integrity of the VHF Data Link (VDL)’ and puts onus on administrations. | Recommends that: any device which transmits on the radio channels allocated for AIS, should meet the appropriate requirements of Recommendation ITU-R M.1371; that all such transmitting devices should be approved by the Administration; and, that Administrations should take the steps necessary to ensure the integrity of the radio channels used for AIS in their waters. |
| IMO | [MSC. Circ.1473](http://www.navcen.uscg.gov/pdf/ais/references/IMO_MSC1_Circ1473_%20Policy_On_Use_Of_AIS_ATON.pdf)  23 May 2014 | Policy On Use Of AIS Aids To Navigation | In Force |  | IMO opted not to use the term synthetic AIS AtoN, but, did not prohibit their use. |
| IMO | SN/Circ.217  11 July 2001 | Interim Guidelines For The Presentation And Display Of AIS Target Information | In Force | Presents the symbol - triangle – for AIS targets | For symbology, also note IHO S57, IALA Rec. V-125 (2003), ISO 19018 (2004) and IEC 62288 (2008) |
| IMO | SN/Circ.227  6 January 2003 | Guidelines For The Installation Of A Shipborne Automatic Identification System (AIS) | In Force (amended by SN/Circ.245) | Details on installation of AIS on board vessels, including interference with VHF, antenna installation, GNSS installation, installation of the unit on the bridge, static and dynamic data input, long range function,. | Issues have arisen with regards to the positioning of the antenna (interference); the quality of the GNSS feed; input of data. |
| IMO | SN/Circ.244 15 Dec 2004 | Guidance on the use of the UN/LOCODE in the destination field in AIS messages | In Force | Adopts the use of UN LOCODE to express the origination and destination of a voyage |  |
| IMO | SN/Circ.227 corr.1  10 Dec 2008 | Corrigenda To SN/Circ.227 On Guidelines For The Installation Of A Shipborne Automatic Identification System (AIS) | In Force  (correction to SN/Circ.227) | Contains changes to ship type, second digit, dangerous cargo. | Developed to reflect the entry into force of resolution MEPC.118(52), concerning the change in the categorization and listing of Noxious Liquid Substances and other substances. |
| IMO | SN/Circ.245  15 Dec 2004 | Amendments To The Guidelines For The Installation Of A Shipborne AIS (SN/Circ.227) | In force (amends SN/Circ.227) | Only change is the inclusion of an uninterrupted power source (UPS) for the AIS. |  |
| IMO | SN/Circ.236  28 May 2004 | Guidance On The Application Of AIS Binary Messages | Superceded | Provides information on the use of the 7 agreed AIS Binary Messages.  Met/Hydro; Dangerous Cargo; Fairway closed; Tidal Window; Extended ship / voyage related data; Number of people on board; Pseudo AIS targets. | The display capability of AIS binary messages is not part of the mandatory functions of the MKD (Minimum Keyboard and Display). The display may require hardware additional to the AIS and dedicated software. After 1 Jan 2013 IMO SN.1/Circ.289 is applied. |
| IMO | SN/Circ.243  15 Dec 2004 | Guidelines For The Presentation Of Navigation-Related Symbols, Terms And Abbreviations | In Force | Provides guidance on the appropriate use of navigation-related symbols to achieve a harmonized and consistent presentation. | Includes presentation of AIS. This circular is references in IEC 62288. |
| IMO | SN.1/Circ.289  2 June 2010 | Guidance On The Use Of AIS Application Specific Messages | In Force | Supersede SN/Circ.236. | There will be significant functionality available for the use of these messages. |
| IMO | SN.1/Circ.290  2 June 2010 | Guidance For The Presentation And Display Of AIS Application-Specific Messages (ASM) Information. | In Force | Provides guidelines on how to present ASM in various formats. | Critical in effectively providing ASM information. |
| IMO | SN/Circ.243 / Rev.1  23 May 2014 | Amended Guidelines For The Presentation Of Navigation-Related Symbols, Terms And Abbreviations | In Force | Provides guidance on the appropriate use of navigation-related symbols to achieve a harmonized and consistent presentation. | Includes presentation of AIS. This circular is references in IEC 62288. |
| IMO | SN/Circ.1473  23 May 2014 | Policy on use of AIS Aids to Navigation | In Force | Defines AIS AtoNs as either Physical or Virtual | Omits the use of synthetic as defined in IALA documents |
| IMO | COMSAR.1/Circ.46  4 Feb. 2009 | AIS Safety-Related Messaging | In Force | Notes issue of using pre-fabricated messages in AIS. | While some units can use pre-set safety related messages (such as can be used in GMDSS, DSC) the system was not designed for such use. |
|  | From IMO web site ([www.imo.org](http://www.imo.org)) | **Maritime security - AIS ship data**  At its79th session in December 2004, the Maritime Safety Committee (MSC) agreed that, in relation to the issue of freely available automatic information system (AIS)-generated ship data on the world-wide web, the publication on the world-wide web or elsewhere of AIS data transmitted by ships could be detrimental to the safety and security of ships and port facilities and was undermining the efforts of the Organization and its Member States to enhance the safety of navigation and security in the international maritime transport sector.  The Committee condemned the regrettable publication on the world-wide web, or elsewhere, of AIS data transmitted by ships and urged Member Governments, subject to the provisions of their national laws, to discourage those who make available AIS data to others for publication on the world-wide web, or elsewhere from doing so.  In addition, the Committee condemned those who irresponsibly publish AIS data transmitted by ships on the world-wide web, or elsewhere, particularly if they offer services to the shipping and port industries. | | | |
| ITU | ITU-R M.1371-5  2014/02 | Technical Characteristics For An Automatic Identification System Using Time Division Multiple Access In The VHF Maritime Mobile Band | Version 5  In Force | Provides the overall technical basis for the working of AIS, including SOTDMA, RATDMA, FATDMA, ITDMA and CSTDMA | ITU recommends that that the AIS design should take into account technical guidelines maintained and published by IALA. |
| ITU | ITU-R M.585-6  2012/01 | Assignment And Use Of Maritime Mobile Service Identities | Version 6  In Force  Note: version 7 will be published in 2015 | Identifies numbering system for MMSIs, | Includes numbering process for ship stations, shore stations, AIS-SART/MOD-AIS/EPIRB-AIS and AIS aids to navigation. |
| ITU | ITU-R M.1842 |  |  |  |  |
| ITU | ITU-R M.2092 |  |  |  |  |
| ITU Documents Are Available For Download From ITU Website [Www.Itu.Int](http://www.itu.int) | | | | | |
| IEC | 61097-14, Ed.1  2010/02 | Global Maritime Distress And Safety System (GMDSS) - Part 14: AIS-SART | In Force | Global maritime distress and safety system (GMDSS) – Part 14: AIS search and rescue transmitter (AIS-SART) | AIS-SART is acceptable for carriage by SOLAS vessels from 1 January 2010 |
| IEC | 61162-1, Ed.4 Ed 4.0  2010/11 | Maritime Navigation And Radiocommunication Equipment And Systems – Digital Interfaces – Part 1: Single Talker And Multiple Listeners | In Force | Contains the requirements for data communication between maritime electronic instruments, navigation and radiocommunication equipment when interconnected via an appropriate system. | Includes AIS presentation interface sentences. (in addition, refer to NMEA 0183) |
| IEC | 61993-2, Ed.3  2012/10 | Part 2:  Class A Shipborne Equipment Of The Universal Automatic Identification System (AIS) – Operational And Performance Requirements | In Force | Provides the actual testing standard for the equipment. Equipment bought should note compliance with this standard.  As part of maintenance cycle, this document is being updated by the IEC AIS Working Group. | Note – 61993-1 is for Shipborne automatic transponder system installation using VHF digital selective calling (DSC) Techniques. |
| IEC | 62287-1, Ed.2.1  2013/04 | Class B Shipborne Equipment Of The  Automatic Identification System (AIS) –Part 1: Carrier-Sense Time Division Multiple Access  (CSTDMA) Techniques | In Force | Provides the actual testing standard for equipment – equipment bought should note compliance with this standard.  Note Politeness factor to accommodate activity on the VDL. | For CSTDMA only. . |
| IEC | 62287-2, Ed.1.0  2013/04 | Class B Shipborne Equipment Of The  Automatic Identification System (AIS) –Part 2: Self-Organising Time Division Multiple Access  (SOTDMA) Techniques | In Force | Testing standard for the equipment. SOTDMA AIS Class B that continues to reflect politeness factor to accommodate activity on the VDL. |  |
| IEC | 62288, Ed.2.0  2015/01 | Presentation Of Navigation-Related Information On Shipborne Navigational Displays | In Force | Specifies presentation of navigational information, including navigational terms, abbreviations, colours and symbols. | Addresses the presentation of information, including the display of AIS units. |
| IEC | 62320-1, Ed.2.0  2015/01 | Part 1: AIS Base Stations - Minimum Operational And Performance Requirements, Methods Of Test And Required Test Results | In Force | Provides the actual testing standard for equipment – equipment bought should note compliance with this standard.  Through implementation of the standard, some corrections have been identified, and a PAS (Publically available standard) is being developed. | Some presentation interface sentences were created for the AIS Base Station, which are being reviewed in the IEC process for inclusion into IEC 61162. Liaison work is underway to resolve PI sentence issues. |
| IEC | 62320-2, Ed.1.0 (2008) | Part 2: AIS Fitted To Aids To Navigation (Aton) | In Force | Introduces concept of three types of AIS, with different functionality. When completed, equipment purchased should note compliance with the standard. | Main difference between types of AIS AtoNs:  Type 1 – no receiver  Type 2 – receiver for control functions only  Type 3 – 2 receiving processes for autonomous mode |
| IEC | 62320-3, Ed. 1.0 (2015) | Part 3: Repeater stations | In Force | specifies the minimum operational and performance requirements, methods of testing and required test results for AIS repeater stations |  |
| IEC Documents are available for purchase from IEC website <http://webstore.iec.ch/webstore/webstore.nsf/artnum/028339> | | | | | |
| IALA | Rec. A-123  June 2007 | On the Provision of Shore Based Automatic Identification Systems (AIS) | In Force – Previous edition Dec. 2003 | A-123 provides high level indication of the need for AIS Base Stations. | This has recently been updated and continues to reflects the overall vision of AIS as presented in SOLAS, Chapter V. Additional reference for Symbology ISO 19018 (2004) |
| IALA | Rec. A-124 Ed. 1.2  Dec. 2003 | On Automatic Identification System (AIS) Shore Station and Networking Aspects relating to the AIS Service | In Force –  under review | The initial concepts of AIS Base Stations, Repeaters and Limited Base Stations. Requires significant revision. | During the process of developing IEC 62320-1 many areas of A-124 were identified for change and a substantial revision is being carried out. |
| IALA | Rec. V-125 Ed. 2  Dec. 2004 | The Use And Presentation Of Symbology At A VTS Centre (Include AIS) | In Force | Provides information on symbology for use at VTS Centres. | Ed. 1 covered AIS aspects only, while Ed. 2 provides a broader view for symbology. |
| IALA | Rec. A-126  June 2007 | The Use Of Automatic Identification Systems (AIS) In Aids To Navigation | In Force / Previous edition Dec. 2003 | Initial information for using AIS as an AtoN | In developing IEC 62320-2 many areas of A-126 were identified for change, and this document represents substantial changes to the initial edition.  A-126 is currently under review. |
| IALA | Rec. V-128 Ed. 3  June 2007 | Operational And Technical performance Requirements For VTS Equipment | In Force | Annex 3 identifies technical requirements for AIS in a VTS centre. | Notes that AIS is a sensor that can be used in VTS. |
| IALA | Rec. O-143  March 2010 | Virtual Aids To Navigation | In Force | Notes application, risks and benefits of virtual aids to navigation. | AIS can be used to transmit virtual aids to navigation. IALA Guideline 1081 provides amplification on the use of virtual aids to navigation. |
| IALA | Guideline 1026  Dec. 2001 | On AIS As A VTS Tool | In Force | Notes how AIS can assist in VTS. | The introduction of AIS in VTS is under review at IALA – an IALA questionnaire is being circulated to gather status of AIS in VTS and to update relevant documents. |
| IALA | Guideline 1028 ed.1.3  Dec. 2004 | On Automatic Identification (AIS) – Volume 1, Part 1 – Operational Issues | In Force / Replaced Guideline 1019 on AIS | Provides information on the actual operation of AIS. | Provides detailed information on how AIS works.  (note – this guideline is no longer being maintained) |
| IALA | Guideline 1029 ed.1.1  Dec 2002 | On Automatic Identification System (AIS) – Volume 1, Part 2 – Technical Issues | In Force / Replaced Guideline 1019 on AIS | Provides information on the technical aspects of AIS  Range formula provided. | Provides detailed technical information, very in-depth on the provision of shore based AIS.  (note – this guideline is no longer being maintained) |
| IALA | Guideline 1032  June 2003 | Aspects Of Training Of VTS Personnel Relevant To The Introduction Of The Automatic Identification System | In Force | Notes the required training for VTS Personnel when AIS is introduced. |  |
| IALA | Guideline 1050  Dec. 2005 | Management And Monitoring Of AIS Information | In Force | Notes the benefits to using AIS in planning and managing aids to navigation systems. | AIS can provide many organisational benefits, both in short term / real time and in long term analysis of data. |
| IALA | Guideline 1059  June 2008 | Comparison Of AIS Stations | In Force | Compares and presents each of the AIS stations. | Will be withdrawn on completion of this document |
| IALA | Guideline 1062  Dec. 2008 | Establishment Of AIS As An Aton | In Force | Identifies possible functions of AIS as an AtoN. | There are benefits to the use of AIS as an AtoN. The impact on the VDL needs to be taken into account. |
| IALA | Guideline 1081  March 2010 | Virtual Aids To Navigation | In Force | Introduces concepts of virtual aids to navigation; user needs; benefits and risks. | Amplifies information presented in Rec. O-143 |
| IALA | Technical Clarifications | Clarifications To ITU-R M.1371 Series | In Force | Created and maintained at the request of ITU. | Technical clarifications to ITU-R M.1371-4 have been developed and liaison between IALA / ITU is underway prior to publishing. |
| IALA | Plan  Dec 2009 | Radio Communications Plan | In Force |  |  |
| IALA | 1095  May 2013 | Implementation of Application–Specific messages | In Force | Intends to aid in harmonisation and establishes the IALA ASM collection | Currently resides at  http://www.e-navigation.nl/asm |
| IALA | 1098  May 2013 | Application of AIS AtoN on buoys | In Force | Provides guidance regarding, specification, installation and maintenance of AIS AtoN on buoys and fixed structures |  |
| IALA Documents available for free download from IALA website [www.iala-aism.org](http://www.iala-aism.org) under ‘publications’ | | | | | |

1. AIS frequently asked questions - http://www.iala-aism.org/products/publications [↑](#footnote-ref-1)
2. Dynamic data is data provided from sensors such as gyro compass, GNSS device or rate of turn indicator; static data refers to data that doesn’t change such as the length or beam of the vessel; voyage related data refers to items such as the vessel draft, port of destination or cargo. [↑](#footnote-ref-2)
3. Radar search and rescue transponders (SART) and AIS-SART are included in the Global Maritime Distress and Safety System (GMDSS). Radar SART are activated by the radar pulse (hence ‘transponder’) while AIS SART transmit at set rates. [↑](#footnote-ref-3)
4. IMO Resolution MSC.74(69) Annex 3. [↑](#footnote-ref-4)
5. IMO Resolution A.917(22). [↑](#footnote-ref-5)
6. Shore authorities should use FATDMA whenever possible instead of RATDMA to avoid slot collisions [↑](#footnote-ref-6)
7. Shore authorities are responsible for the allocation and reservation of FATDMA slots. [↑](#footnote-ref-7)
8. Ch. 87B (AIS1) and Ch. 88B (AIS2). [↑](#footnote-ref-8)
9. FATDMA slot allocation should be coordinated amongst administrations, reference IALA Recommendation A-124 (Annex 14). [↑](#footnote-ref-9)
10. Regional registry <http://vislab-ccom.unh.edu/~schwehr/ais/collection/> (also accessible from the IALA website at [www.iala-aism.org](http://www.iala-aism.org) under ‘services offered’). [↑](#footnote-ref-11)
11. Refer to IMO Resolution MSC140(76) Recommendation for the protection of the AIS VHF data link. [↑](#footnote-ref-12)
12. Refer to IALA Recommendation A-124 Annex 17. [↑](#footnote-ref-13)
13. Inland AIS as used in inland waterways is a derivative of Class A. [↑](#footnote-ref-14)
14. While Class A initially had a low-power of 2 watts, this was amended in a subsequent edition of ITU-R M.1371-3. The main issue that this change addressed was the requirement for limitations in power as identified in the International Safety Guide for Oil Tankers and Terminals (ISGOTT), fifth edition. [↑](#footnote-ref-17)
15. IMO Resolution MSC.246(83). [↑](#footnote-ref-18)
16. Reference IALA Guideline 1062 on the establishment of AIS as an aid to navigation and IALA Recommendation A-126 on AIS as an AtoN. [↑](#footnote-ref-19)