

**IALA RECOMMENDATION**

R0146 (e-NAV-146)

STRATEGY FOR MAINTAINING RACON SERVICE CAPABILITY

**Edition 2.0**

**Oct, 2024**

**urn:mrn:iala:pub:r0146**

Revisions to this document are to be noted in the table prior to the issue of a revised document.

|  |  |  |
| --- | --- | --- |
| **Date** | **Details** | **Approval** |
| December 2011 | 1st issue |  |
| September 2020 | Edition 1.1 Editorial corrections. |  |
| Oct 2024 | Edition 2.0 |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**THE COUNCIL**

**RECALLING** the function of IALA with respect to Safety of Navigation, the efficiency of maritime transport and the protection of the environment;

**RECOGNIZING** that radar will continue to have an important role in hazard warning, spatial awareness and confirmation of position;

**RECOGNIZING ALSO** that a racon service assists in position determination by providing a readily identifiable radar target;

**RECOGNIZING FURTHER** the anticipated continuing requirement for racons in the e-Navigation era;

**NOTING** that IMO have approved new radar performance standards which from 1 July 2008 removed the requirement for S-Band radars to trigger Racons;

**NOTING ALSO** that solid-state S-Band radars offer benefits of improved radar detection performance utilising lower peak power than conventional radar;

**NOTING FURTHER** that solid-state S-Band radars are being offered by manufacturers and are being fitted on ships;

**NOTING FURTHER** that IMO continues to recognize the importance of racons as an aid to navigation;

**CONSIDERING** that National Members and other appropriate authorities wish to maintain their racon service capability, and the benefits to navigation that accrue from these services;

**ADOPTS** the strategy in the annex to this recommendation; and,

**RECOMMENDS** that National Members and other appropriate Authorities providing marine aids to navigation services follow the strategy as detailed in section 6 of the annex.

**ANNEX A STRATEGY FOR MAINTAINING RACON SERVICE CAPABILITY** [**5**](#bookmark1)

**1 INTRODUCTION** [**5**](#bookmark2)

**2 PRESENT SITUATION** [**5**](#bookmark3)

**3 TECHNICAL BACKGROUND** [**5**](#bookmark4)

**4 THE ROLE OF RACONS** [**6**](#bookmark5)

**5 OPTIONS FOR RACON SERVICES** [**7**](#bookmark6)

5.1 Use Existing Racons [7](#bookmark7)

5.2 Improve Existing Racons [7](#bookmark8)

5.3 Enhanced Racons [7](#bookmark9)

5.4 Universal Radar Beacon [7](#bookmark10)

5.5 Secondary Radar [7](#bookmark11)

5.6 Non-radar technology [7](#bookmark12)

**6 THE STRATEGY** [**8**](#bookmark13)

**7 REFERENCES** [**8**](#bookmark14)

**List of Tables**

*Table 1 Comparison of characteristics of conventional and typical NT radars*  [*6*](#bookmark15)

**ANNEX A STRATEGY FOR MAINTAINING RACON SERVICE CAPABILITY**

**1 INTRODUCTION**

This strategy deals with the anticipated developments in solid-state radar over the next decades, the consequences for existing racon performance with a potential reduction in the racon service capability, and the requirement to update racon for meeting this challenge. The strategy reflects discussions in IALA and consultation with other bodies such as CIRM. Any regulatory changes considered necessary will need to be coordinated through IALA and progressed in IMO, ITU and IEC, as appropriate.

**2 PRESENT SITUATION**

The advent of solid-state radar, with low power, solid-state transmitters introduces uncertainty about the future of Racons.

In 2004, IMO MSC79 approved new radar performance standards in Resolution 192(79), which from 1 July 2008 removed the requirement for S-Band radars to trigger Racons. This was intended to facilitate the introduction of cost effective coherent processing techniques that would enable future radars to have an improved performance in sea and rain clutter. Potentially, it also allowed more stringent limits to be considered by ITU on spurious and out of band emissions of marine radars in order to improve the utilisation efficiency of the radar spectrum.

S-Band radar is normally the preferred choice by users when operating in adverse conditions, particularly in open waters, when the extra angular resolution of X-Band radar is not so important. S-Band is much less affected by precipitation clutter than X-Band. IMO saw that the potential performance improvements that could be obtained by using new technology (NT) would therefore be particularly beneficial at S-Band. The requirement to trigger Racons was dropped in order not to limit the possibilities of improving radar performance in clutter. However, IMO continues to recognize the importance of Racons as an aid to navigation, since they provide a means of identifying and locating navigation marks in poor visibility without reliance on GNSS or other electronic position fixing systems. For this reason the requirement at X-Band on Racon compatibility has not been altered.

Prior to IMO’s decision, the Nautical Institute carried out a survey of bridge officers and established that there was a consensus on an approach that effectively trades S-Band Racon compatibility for improved radar detection in conditions of heavy clutter. New systems and services provide an ever-increasing array of options through which to optimise service levels and reduce risk and cost. At the same time, the need for co-ordination through IALA and key stakeholders such as IMO and CIRM has never been more important in the endeavour to ensure consistent levels of service provision on an international basis.

Recognising the benefits of improved radar detection performance resulting from solid-state radar, and the relatively small number of racons compared with the number of radars installed worldwide, it is necessary for service providers to consider updating of racon if the racon service is to be maintained.

**3 TECHNICAL BACKGROUND**

Solid-state S-Band radar solutions have already emerged over the past years and that these will rapidly be adopted by users and manufacturers. These may include solid state amplifiers, pulse compression, Travelling Wave Tube or Frequency Modulation Carrier Wave (FMCW). Target and clutter Doppler information may be used to enhance target visibility; in fact these techniques may also be used with magnetron radars. There are however, several benefits with the low peak powers resulting from pulse compression techniques, which enable solid-state transmitters to be used. The required technology has become increasingly affordable because of the escalating market for mid-power microwave digital communication systems.

Solid-state transmitters also allow the easy use of frequency diversity techniques, giving a further significant boost to target detectability. They offer good benefits in improving the reliability of radar systems compared to

magnetron based systems. Magnetrons have a limited in-service life (c10,000 hours) and require very high voltage power supplies that limit reliability.

*Table 1 Comparison of characteristics of conventional and typical NT radars*

|  |  |
| --- | --- |
| **Conventional Radar** | **Solid-state Radar** |
| non-coherent | coherent |
| pulsed | modulated pulse |
| high peak power (3-30 kW) | low peak power (10-500 W) |
| magnetrons | solid-state |

Note that the interaction of FMCW radars and racons requires a completely new approach to be developed. This has not been considered as part of this strategy paper.

**4 THE ROLE OF RACONS**

This Strategy is set in the following context:

• radar will continue to be the primary tool for collision avoidance for the foreseeable future;

• radar will continue to have an important role in hazard warning, spatial awareness and confirmation of position;

• anticipated continuing requirement for Racons in the e-Navigation era;

• the navigational requirement for Racons in the future is expected to be as set out in Appendix 1;

• there is a need to respond to the proliferation of other radar targets, such as wind farms;

• increasing congestion in some areas is making greater demands on AtoN; and

• radars may be introduced over the next decades that will not trigger existing racons, or will do so at significantly reduced range.

Mariners have access to a rapidly increasing amount of information, bringing with it a risk of information overload, which needs to be addressed under the Human-Machine Interface aspects of e-Navigation. This necessitates an ability to interpret and discriminate between individual aids to navigation in an environment with an increasing amount of radar clutter. There is a potential single point of failure with both the navigation and surveillance functions of bridge systems relying solely on GNSS. Radar aids to navigation are, and will remain, a key part of the approach to risk mitigation.

The removal of the requirement to trigger racons does not necessarily mean that racons will not work with solid-state radars. They may work at a reduced, but acceptable range; Solid-state radars could be designed to trigger racons, whilst retaining their other performance advantages; alternatively, existing racons could be modified to work with solid-state radars or new racons designed to do so. Calculations of performance with early solid-state radars indicate that existing racons will perform, but with reduced range.

Trials have been carried out with a solid-state radar, which have indicated a serious reduction in range with most existing racons (References [1] & [2]). These trials have indicated the need for the development of this strategy.

Solid-state radars are only being introduced at S-Band at present for SOLAS vessels, although there are X-Band solid-state radars available for non-SOLAS vessels. If X-Band solid-state radars are effective in improving small target detection in clutter it is likely that demand will grow for their application to SOLAS vessels. However, it is not currently anticipated that IMO will allow significant relaxation of the X-Band radar requirements to trigger and display racons.

The important role of racons is being challenged at S-Band and in the longer term at X-Band. As a result, the development of a suitable strategy for both S-Band and X-Band Racon services is considered vital.

**5 RACON SERVICES**



To consider the design of a universal racon that would be compatible with all types of conventional and solid-state radars. In principle, this is possible using main-stream advances in digital microwave techniques, digital RF memory and fast DSP. Although it stretches today’s technology, it is likely that future advances will make this approach affordable. Its main advantage is that it is potentially compatible with all present and future radars. Racon power consumption would be a major consideration. r

**6 THE STRATEGY**

IALA members should present the case for retaining the existing racon service capabilities in X-Band radar developments, are encouraged to provide S-Band racon services optimised for conventional and solid-state radars.

Recognising the benefits of improved radar detection performance resulting from pulsed solid-state radar, a universal racon should be considered when planning a replacement or upgrade of equipment to maintain and enhance service capability.

IALA members are encouraged to support and consider the possibility of the universal racon in the longer term.

IALA should encourage liaison with radar manufacturers to confirm that solid-state radars have the capacity to trigger racons at the proposed ranges, and work with racon manufacturers to identify possible modification to improve triggering range.

**7 REFERENCES**



[1] RPT-06-MB-09 Racon Trials, GLA R&RNAV 2010

[2] RPT-07-NW-10 Second Racon Trials, GLA R&RNAV 2010

**APPENDIX 1 PROPOSED NAVIGATIONAL REQUIREMENT FOR RACONS**

**1. BACKGROUND**



Racons are an important element of the present and future AtoN mix.

IALA Recommendations / Guidelines and the NAVGUIDE set out the following typical uses of Racons:

• Inconspicuous coastlines.

• Ice conditions.

• Identification of AtoN at long range.

• Landfall identification.

• Traffic Separation Scheme / precautionary area.

• Hazard marking.

• Navigable spans under bridges.

• Leading lines.

• Short range Racon identification of a local feature (e.g. a harbour entrance).

• New Dangers (Morse D).

• Offshore structures.

• Turning Marks.

• ERPS and MASS

In the absence of any specific considerations IALA recommends that the availability of a racon should be at least 99.6%, however many authorities treat all racons as Category 1 AtoN with an availability target of 99.8%.

**2. REQUIRED RACON RANGE**



Racon range will depend on a number of factors including transmitter power, height of the racon and height of radar. The Admiralty List of Radio Signals Volume 2 sets out the approximate ranges of Racons presently provided as well as some general information on Racon performance. At present racon ranges are set out in two formats, in some cases a single range is given and in others a spread of ranges is given.

It is proposed that the navigational requirements for racon range (regardless of radar type) should be a minimum of 5 nautical miles from a floating AtoN and 10 nautical miles from a fixed AtoN. These figures are based on a typical height of racon of 5 metres for floating and 20 metres for fixed racons and a radar height of 20 metres.

This performance level ignores the effect of fading due to multi-path interference, the impact of which will vary with the heights of antennas above sea level and with sea state.

**3. RELATED DOCUMENTATION**



IALA Guideline G1010 Racon range performance.

IALA Recommendation R0101 (R-101) Maritime Radar Beacons (Racons). IALA Recommendation R0113 (O-113) for the marking of fixed bridges.

IALA Guideline G1147 The Use of Enhanced Radar Positioning Systems

IALA NAVGUIDE.

IMO Resolution MSC.192(79) – Radar Performance Standards.

Admiralty List of Radio Signals Volume 2, UK Hydrographic Office.