|  |  |
| --- | --- |
| From: e-Nav Committee | ANM15/9/4  Formerly e-NAV8/output/11 |
| To: ANM Committee | 24 September 2010 |

Liaison Note

**Procedure for the Authorisation of AIS AtoN**

**Template for AtoN application**

# Background

The document ANM14/output/4 sets out a protocol for the authorisation of AIS AtoN. The e-NAV Committee considered the document and agrees with the main structure identified. Modifications are shown in track changes.

In addition, the e-NAV Committee developed a template to assist those authorising the provision of AIS AtoN.

# Proposed procedure for the Authorisation of AIS AtoNs

## Introduction

AIS can be used as an Aid to Navigation (AtoN) and may be deployed by the maritime administration or other organisations, such as local AtoN authorities or offshore energy companies. Maritime administrations including lighthouse authorities generally have a statutory obligation to provide marine aids to navigation in their coastal waters and to supervise their deployment by other organisations.

However, AIS AtoNs require a radio licence and the radio licensing authority may be different from the maritime administration. In such cases there may be a need for a coordinated procedureto ensure that AIS AtoNs are correctly licensed and authorised, without unnecessarily delaying or obstructing their deployment. The attached AIS AtoN Specification Sheet is provided to assist in this application process. In some cases international consultation may be necessary to ensure coordination of slot allocations.

The authorities involved can be diverse and include Marine Administrations, Coast Guards, Communications Regulators, Hydrographic Services, Lighthouse Authorities and other governmental and non governmental organisations and agencies. In some cases the IALA National Member will be the authority but in others non IALA members will be involved.

## Procedure

Where a single authority has responsibility for all aspects of the application the normal procedures can be followed, bearing in mind possible implications for adjacent countries.

Where different authorities are responsible for the AtoN and radio aspects of the application the following procedure is proposed.

The authorities should agree in advance who has responsibility for:

* allocation of MMSI;
* ITU reporting; and
* AIS Slot map allocations for the different types of AIS transmitter (base station, mobile, AtoN, SART, etc).

It is assumed in the example below that slots are allocated by the maritime administration and MMSI by the radio licensing authority. This may differ from country to country.

In addition the parties should agree timescales for turnaround of applications and a communication protocol at each stage. Electronic circulation of documentation may speed up the process.

### Stage 1 – Receive application

When any licensing authority receives an AIS AtoN application, the receiving authority should forward copies to other relevant authorities.

### Stage 2 – Review application

The authorities involved should confirm that all aspects of the AIS AtoN specification sheet have been addressed. The lighthouse authority or other relevant body should determine if the proposed AIS AtoN:

* is appropriate in the general mix of AtoNs for the area concerned
* does not impose undue loading on the VDL
* operation will be monitored (i.e. by another base station, as part of a network)
* confirms optimum slot allocation scheme (if FATDMA, confirm slot availability and reservations)

During the review process it may be necessary to coordinate with other competent authorities in the region due to the proposed location.

### Stage 3 – Approve / Deny application

Any application for an AtoN should be approved by the lighthouse authority and/or other relevant body prior to radio licensing.

The application will then be returned to the applicant advising approval, approval with qualifications/changes, or deny. In the case of applications that have been denied, reasonable explanation should be given noting that it may be possible to re-apply with revised parameters.

Approved applications should include the identified MMSI and, if required, the allocated fixed access timeslots.

It is important that the MMSI be assigned in accordance with Recommendation ITU-R M.585-5 and that the procedures set out in ITU Circular Letter CM/17 be followed to ensure that the MMSI is recorded on the ITU database.

At each stage of the process all other authorities involved should be kept informed.

A single notice of approval to the applicant containing all required permissions is preferred. However, where this is not possible, individual notifications may be submitted.

Authorities should implement procedures to ensure approved AIS AtoNs operate according to the parameters in their authorisation.

AIS AtoN Specification Sheet

|  |  |  |
| --- | --- | --- |
| **Applicant Details** | | |
|  | Applicant / Owner | Operator (if different) |
| Contact Name |  |  |
| Organization |  |  |
| Contact Details  Address |  |  |
| Phone |  |  |
| Mobile |  |  |
| e-mail |  |  |

| **Message 21 content** | | |
| --- | --- | --- |
| **Parameter** | values | Comment / description |
| Maritime Mobile Service Identity (MMSI) |  | Provided by Competent Authority issuing the MMSI  [See IALA web page for contact information of national competent authority] |
| Name of AtoN |  | Denote AtoN Name up to 34 characters |
| Nature and Type of AtoN |  | Denote the type of AtoN; see IALA A-126 |
| Synthetic and Virtual AtoN |  | If unit is transmitting virtual or synthetic specify message 21 content (e.g. MMSI, position, etc), reporting interval, channel.  A separate form for each synthetic or virtual AtoN message should be attached |
| Dimension/ Reference for Position | A=  B=  C=  D= |  |
| Type of electronic position fixing device |  | 0 = Undefined (default) 1 = GPS 2 = GLONASS 3 = Combined GPS/GLONASS 4 = Loran-C 5 = Chayka 6 = Integrated Navigation System  7 = surveyed. For fixed AtoN and virtual AtoN, the charted position should be used. The accurate position enhances its function as a radar reference target 8 = Galileo 9-14 = not used  15 = internal DGNSS |
| AtoN status |  | Denote status indicators available on the AtoN  See IALA A-126 |
| **Supplemental information** | | |
| Intended Position |  | The position where the AtoN will be deployed |
| Process for deployment |  | Indicate how and who will be deploying the unit |
| Off-position Threshold |  | Denote off-position threshold expressed in meter,  see IALA A-126 |
| RAIM capability |  | Denote whether EPFS has RAIM capability |
| Access Mode for Message 21 |  | FATDMA, RATDMA or both.  If FATDMA: denote slots provided by Competent Authority for VDL slot management  [See IALA web page for contact information of national competent authority] |
| Date of Certification |  | Provide the date of type certification to IEC 62320-2 |
| **Other messages** | | |
| Additional messages |  | Additional messages 6, 8, 12, 14 or other appropriate messages possible, but, must be denoted here. Application Specific Message should provide DAC and FI as registered with IALA. |
| Content of message 12 and 14 |  | Provide the text |
| Access Mode for Messages other than 21, if implemented |  | FATDMA, RATDMA and/or CSTDMA. If FATDMA specified, state slots used. |

|  |  |  |
| --- | --- | --- |
| **Message scheduling** | | |
| **Parameter** | values | Comment / description |
| Messages Transmitted / Reporting interval per channel | 21: every \_\_ minutes/channel a / b  Other messages (include DAC/FI):  every \_\_ minutes/channel a / b | Message 21 transmission required minimum every X minutes; additional messages 6, 8, 12, 14 or other appropriate messages possible, but, must be denoted here. Application Specific Message should provide DAC and FI. |
|  |  |  |
|  |  |  |
| **Physical attributes of AIS AtoN Station** | | |
| AIS AtoN Station Type |  | Denote AIS AtoN Station Type (i.e. 1, 2, 3); see IALA Recommendation A 126  Denote No Receiver (Type 1), Receiver for control functions only (Type 2), or Receiving processes for autonomous mode (Type 3) |
| Configuration method |  | Denote whether via the VDL and or proprietary.  Provide further information, e.g.  + Standard PI sentences (IEC 61162)  + Standard AIS AtoN binary configuration messages  + Proprietary sentences  + Proprietary binary configuration messages |
| Transmit Power |  | + default (12.5 W)  + or as defined by manufacturer and denoted here |
|  |  |  |
| Power availability |  | Denote power source: main or auxiliary e.g. power grid, |
| Transmitter capability |  | Denote whether dual or single channel (Type 1 and 2 only) |
| Receiver availability |  | Denote receiver on times |
| UTC synchronisation |  | Denote either Direct, Indirect or semaphore (Types 3) |
| Chaining |  | If capable provide all MMSIs in the chain and the neighbouring AIS AtoN station (parent and child) of this station in the chain |