ANM19/47

Formerly EEP19/output/10

**Table 9 – Maximum period for rhythmic characters of aids to navigation lights**

|  |  |
| --- | --- |
| Character Class | Maximum period  (seconds) |
| Isophase light | 12 |
| Single-occulting light | 15 |
| Single-flashing light | 15 |
| Group very quick light | 15 |
| Group-occulting light of two eclipses | 20 |
| Long-flashing light | 20 |
| Group-flashing lights of two flashes | 20 |
| Group-quick light | 20 |
| Group-occulting light of three or more eclipses | 30 |
| Group-flashing light of three or more flashes | 30 |
| Composite group-flashing light | 30 |
| Morse code light | 30 |