|  |  |
| --- | --- |
| From: ENG Committee | ARM7-8.2.7 (ENG7-11.1.31) |
| To: ARM Committee | 13 October 2017 |

LIAISON NOTE

MOBILE ATON

# Introduction

The ENG Committee was requested to respond to the request from ARM on the development of the marking of Mobile ATON. The Committee considered this and responds as follows:-

The use of a single conspicuous light character would be desirable for this application to avoid confusion.

The ENG Committee suggests a yellow light with Morse ‘D’ character defined as:-

2.1s (fl) + 0.7s (ec) + 0.7s (fl) + 0.7s (ec) + 0.7s (fl) + 6.3s (ec)

Mo(D) Y

The additional of ‘flicker’ (strobe effect) in the smaller flashes would increase conspicuity at close range.

This and other characters will be demonstrated to the ARM Committee at ARM7.

# Action requested

The ARM Committee is requested to consider the above suggestion and advise on their decision.