Reference: ENG4-11.1.9

# Purpose

This document should be used to submit proposals for additions, amendments or deletions of terms in the International Dictionary of Marine Aids to Navigation (Dictionary). Proposals will be considered by the Dictionary Working Group (DWG) of the IALA Policy Advisory Panel (PAP) and the Dictionary will be amended if the proposal(s) is approved.

# Proposed amendment of the Dictionary

Please use the following table to submit proposals for additions, amendments or deletions of terms in the Dictionary.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Term** | **Dictionary Number** | **Source**  **(meeting/**  **document/**  **person)** | **Old definition** | **Proposed definition**  **English** | **Reason for change** | **Date** | **Accept**  **Reject** |
| Sector Accuracy |  | ENG4  Guideline 1041 | NONE | Sector accuracy is the maximum angle between the intended sector boundary and the actual sector boundary. | New definition | 2016-04-12 |  |
| Alternating Sector |  | ENG4  Guideline 1041 | NONE | An alternating sector is a sector with alternating flashing colours of fixed flash length throughout the sector. | New definition | 2016-04-12 |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |