**Alternative solution to remove Mercury keeping the existing lens**

In order to eliminate the hazards associated with mercury, keeping the existing historical lens, an alternative solution exists. A new ball revolving pedestal can be installed on the existing pedestal, after complete removal of mercury. This solution has been selected and installed by CETMEF (France) for Lighthouses in the French West Indies.

