|  |  |
| --- | --- |
| From: ENG Committee | ENG7-11.1.31 |
| To: ARM Committee | 13 October 2017 |

LIAISON NOTE

MOBILE ATON

# Introduction

The ENG Committee were requested to respond to the request from ARM on the development of the marking of MATON. The Committee considered this and respond in the following manner:-

The use of a single conspicuous light character would be desirable for this application to avoid confusion.

WG1 of the ENG Committee suggests a Morse ‘D’ character defined as:-

2.1s (fl) + 0.7s (ec) + 0.7s (fl) + 0.7s (ec) + 0.7s (fl) + 6.3s (ec)

Mo(D) Y

The additional of ‘flicker’ (strobe effect) in the smaller flashes would increase conspicuity at close range.

This and other characters will be demonstrated to the ARM Committee at ARM7.

# Action requested

The ARM Committee is requested to consider the above suggestion and advise on their decision.